{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":53,"n_cols":6,"rows_kept":53,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTA-BW"]
[]
[]
[]
[]
["","","","","","FTXTA30B2V1BW"]
["Garso slėgio lygis","Šildymas","","Aukštas","dBA","41"]
["","","","Vidutinis","dBA","31"]
["","","","Tylus veikimas","dBA","19"]
["","","","Žemas","dBA","24"]
["","Aušinimas","","Vidutinis","dBA","32"]
["","","","Tylus veikimas","dBA","20"]
["","","","Žemas","dBA","25"]
["","","","Aukštas","dBA","43"]
["Standartiniai priedai","Įrengimo vadovas","","","","1"]
["","Eksploatavimo vadovas","","","","1"]
["","Oro filtras","","","","2"]
["","Infraraudonųjų spindulių nuotolinio valdymo pultelis","","","","1"]
["","Nuotolinio valdymo valdiklio montavimo plokštė","","","","1"]
["","Sraigto maišas","","","","1"]
["","Sraigto apdangalas","","","","2"]
["","AAA sausosios baterijos","","","","2"]
["","Bendrosios saugos priemonės","","","","1"]
["Šaltnešis","GWP","","","","675.0"]
["Control systems","Wired remote control","","","","BRC073A4"]
["","Infrared remote control","","","","ARC466A59"]
["Vamzdžių jungtys","Skystis","","OD","mm","6.35"]
["","Dujos","","Iš. diam.","mm","9.50"]
["","Drain","","","","18"]
["Tiekiama galia","Aušinimas","","Nom.","kW","0.023"]
["","Šildymas","","Nom.","kW","0.022"]
["Garso galingumo lygis","Vėsinimas","","","dBA","60"]
["","Šildymas","","","dBA","60"]
["Matmenys","Įrenginys","","Plotis","mm","798"]
["","","","Gylis","mm","189"]
["","","","Aukštis","mm","295"]
["Korpusas","Colour","","","","Balta spalva"]
["Svoris","Įrenginys","","","kg","11.5"]
["Ventiliatorius","Oro srauto koef.","Šildymas","Didelis","m³/min.","11.5"]
["","","","Mažas","m³/min.","6.0"]
["","","","Vidutinis","m³/min.","8.0"]
["","","","Tylus veikimas","m³/min.","5.1"]
["","","Aušinimas","Mažas","m³/min.","5.7"]
["","","","Vidutinis","m³/min.","8.3"]
["","","","Didelis","m³/min.","11.9"]
["","","","Tylus veikimas","m³/min.","4.6"]
["Power supply","Phase","","","","1~"]
["","Dažnis","","","Hz","50"]
["","Pavadinimas","","","","V1"]
["","Įtampa","","","V","220-240"]
["Pastabos","","","","","(1) - Aušinimas: vidaus temp. 27 °CDB, 19,0 °CWB; lauko temp. 35 °CDB, 24 °CWB; ekvivalentinis vamzdyno ilgis: 5 m"]
["","","","","","(2) - Šildymas: vidaus temp. 20 °CDB; lauko temp. 7 °CDB, 6 °CWB; ekvivalentinis aušinimo medžiagos vamzdyno ilgis: 5 m"]
["","","","","","(3) - Žr. atskirą elektros duomenų brėžinį"]