{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":7,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-M"]
[]
[]
[]
[]
["","","","","","FTXTM30M2V1B","FTXTM40M2V1B"]
["Tiekiama galia","Aušinimas","","Nom.","kW","0.032","0.037"]
["","Šildymas","","Nom.","kW","0.037","0.04"]
["Korpusas","Spalva","","","","Balta","Balta"]
["Matmenys","Įrenginys","","Aukštis","mm","294","300"]
["","","","Plotis","mm","811","1040"]
["","","","Gylis","mm","272","295"]
["Svoris","Įrenginys","","","kg","10","14.5"]
["Ventiliatorius","Oro debitas","Aušinimas","Didelis","m³/min.","11.7","15.5"]
["","Oro srauto greitis","Vėsinimas","Vidutinis","m³/min.","8","9.2"]
["","","","Mažas","m³/min.","6.3","5.7"]
["","","","Tylus veikimas","m³/min.","5.2","4.6"]
["","","Šildymas","Didelis","m³/min.","12.2","17.7"]
["","Oro srauto greitis","Šildymas","Vidutinis","m³/min.","7.5","11"]
["","","Šildymas","Mažas","m³/min.","5.1","7.5"]
["","","","Tylus veikimas","m³/min.","4.1","6.3"]
["Garso galingumo lygis","Vėsinimas","","","dBA","60","60"]
["","Šildymas","","","dBA","61","61"]
["Garso slėgio lygis","Aušinimas","","Aukštas","dBA","45","46"]
["","Vėsinimas","","Vidutinis","dBA","33","32"]
["","","","Žemas","dBA","25","24"]
["","","","Tylus veikimas","dBA","21","20"]
["","Šildymas","","Aukštas","dBA","45","46"]
["","","","Vidutinis","dBA","31","31"]
["","","","Žemas","dBA","22","22"]
["","","","Tylus veikimas","dBA","19","19"]
["Vamzdžių jungtys","Skystis","","OD","mm","6.35","6.35"]
["","Dujos","","Iš. diam.","mm","9.5","9.5"]
["","Drenažas","","","","16 (jungiamosios žarnos vidinis diametras)","16 (jungiamosios žarnos vidinis diametras)"]
["Valdymo sistemos","Nuotolinis infraraudonųjų spindulių pultelis","","","","ARC466A55","ARC466A55"]
["","Laidinis nuotolinio valdymo pultelis","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["El. tiekimas","Pavadinimas","","","","V1","V1"]
["","Fazė","","","","1~","1~"]
["Maitinimas","Dažnis","","","Hz","50","50"]
["","Įtampa","","","V","220-240","220-240"]