{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":94,"n_cols":7,"rows_kept":94,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-R"]
[]
[]
[]
[]
["","","","","","FTXTM30R2V1B","FTXTM40R2V1B"]
["Garso slėgio lygis","Šildymas","","Aukštas","dBA","45.0"]
["","","","Vidutinis","dBA","31.0"]
["","","","Tylus veikimas","dBA","19.0"]
["","","","Žemas","dBA","22.0"]
["","Aušinimas","","Vidutinis","dBA","33.0"]
["","","","Tylus veikimas","dBA","21.0"]
["","","","Žemas","dBA","25.0"]
["","","","Aukštas","dBA","45.0"]
["Standartiniai priedai","Įrengimo vadovas","","","","1"]
["","Eksploatavimo vadovas","","","","1"]
["","Belaidis nuotolinis valdymas","","","","1"]
["","AAA sausosios baterijos","","","","2"]
["","Nuotolinio valdymo pulto laikiklis","","","","1"]
["","Pritvirtinimo plokštė","","","","1"]
["","Vidinės įrangos pritvirtinimo varžtai","","","","2"]
["","Sidabrinis dalelių filtras","","","","1"]
["Control systems","Wired remote control","","","","BRC073A1"]
["","Infrared remote control","","","","ARC466A75"]
["Vamzdžių jungtys","Skystis","","OD","mm","6.35"]
["","Dujos","","Iš. diam.","mm","9.50"]
["","Drenažas","","","","18"]
["Tiekiama galia","Aušinimas","","Nom.","kW","0.035"]
["","Šildymas","","Nom.","kW","0.039"]
["Garso galingumo lygis","Vėsinimas","","","dBA","60.0"]
["","Šildymas","","","dBA","61.0"]
["Matmenys","Įrenginys","","Plotis","mm","778"]
["","","","Gylis","mm","272"]
["","","","Aukštis","mm","295"]
["Korpusas","Colour","","","","Balta spalva"]
["Svoris","Įrenginys","","","kg","10.0"]
["Ventiliatorius","Oro debitas","Šildymas","Didelis","m³/min.","12.5"]
["","","","Mažas","m³/min.","4.9"]
["","","","Vidutinis","m³/min.","7.5"]
["","","","Tylus veikimas","m³/min.","4.0"]
["","","Aušinimas","Mažas","m³/min.","5.3"]
["","","","Vidutinis","m³/min.","7.8"]
["","","","Didelis","m³/min.","12.2"]
["","","","Tylus veikimas","m³/min.","4.1"]
["Power supply","Phase","","","","1~"]
["","Dažnis","","","Hz","50"]
["","Pavadinimas","","","","V1"]
["","Įtampa","","","V","220-240"]
["Pastabos","","","","","(1) - Aušinimas: vidaus temp. 27 °CDB, 19,0 °CWB; lauko temp. 35 °CDB, 24 °CWB; ekvivalentinis vamzdyno ilgis: 5 m"]
["","","","","","(2) - Šildymas: vidaus temp. 20 °CDB; lauko temp. 7 °CDB, 6 °CWB; ekvivalentinis aušinimo medžiagos vamzdyno ilgis: 5 m"]
["","","","","","(3) - Žr. atskirus elektros duomenų brėžinius"]
["Tiekiama galia","Aušinimas","","Nom.","kW","","0.053"]
["","Šildymas","","Nom.","kW","","0.06"]
["Korpusas","Spalva","","","","","Balta"]
["Matmenys","Įrenginys","","Aukštis","mm","","299"]
["","","","Plotis","mm","","998"]
["","","","Gylis","mm","","292"]
["Svoris","Įrenginys","","","kg","","14.5"]
["Ventiliatorius","Oro debitas","Aušinimas","Didelis","m³/min.","","15.4"]
["","Oro srauto greitis","Vėsinimas","Vidutinis","m³/min.","","9.5"]
["","","","Mažas","m³/min.","","5.8"]
["","","","Tylus veikimas","m³/min.","","4.6"]
["","","Šildymas","Didelis","m³/min.","","17.5"]
["","Oro srauto greitis","Šildymas","Vidutinis","m³/min.","","10.5"]
["","","Šildymas","Mažas","m³/min.","","7.1"]
["","","","Tylus veikimas","m³/min.","","5.9"]
["Garso galingumo lygis","Vėsinimas","","","dBA","","60"]
["","Šildymas","","","dBA","","61"]
["Garso slėgio lygis","Aušinimas","","Aukštas","dBA","","46"]
["","Vėsinimas","","Vidutinis","dBA","","32"]
["","","","Žemas","dBA","","24"]
["","","","Tylus veikimas","dBA","","20"]
["","Šildymas","","Aukštas","dBA","","46"]
["","","","Vidutinis","dBA","","31"]
["","","","Žemas","dBA","","22"]
["","","","Tylus veikimas","dBA","","19"]
["Vamzdžių jungtys","Skystis","","OD","mm","","6.35"]
["","Dujos","","Iš. diam.","mm","","9.5"]
["","Drenažas","","","","","18"]
["Control systems","Infrared remote control","","","","","ARC466A75"]
["Valdymo sistemos","Laidinis nuotolinio valdymo pultelis","","","","","BRC073A1"]
["Standartiniai priedai","Installation manual","","","","","1"]
["","Wireless remote control","","","","","1"]
["","AAA dry-cell batteries","","","","","2"]
["","Operation manual","","","","","1"]
["","Titanium apatite deodorizing filter","","","","","1"]
["","Silver particle filter","","","","","1"]
["","Indoor unit fixing screws","","","","","2"]
["","Mounting plate","","","","","1"]
["","Remote control holder","","","","","1"]
["El. tiekimas","Pavadinimas","","","","","V1"]
["","Fazė","","","","","1~"]
["Maitinimas","Dažnis","","","Hz","","50"]
["","Įtampa","","","V","","220-240"]