{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":7,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTP-N"]
[]
[]
[]
[]
["","","","","","FTXTP25N5V1B","FTXTP35N5V1B"]
["Tiekiama galia","Aušinimas","","Nom.","kW","0.032","0.032"]
["","Šildymas","","Nom.","kW","0.032","0.032"]
["Korpusas","Spalva","","","","Balta","Balta"]
["Matmenys","Įrenginys","","Aukštis","mm","286","286"]
["","","","Plotis","mm","770","770"]
["","","","Gylis","mm","225","225"]
["Svoris","Įrenginys","","","kg","9","9"]
["Ventiliatorius","Oro debitas","Aušinimas","Didelis","m³/min.","11","11"]
["","Oro srauto greitis","Vėsinimas","Vidutinis","m³/min.","7.9","7.9"]
["","","","Mažas","m³/min.","5","5"]
["","","","Tylus veikimas","m³/min.","3.7","3.7"]
["","","Šildymas","Didelis","m³/min.","10.5","10.5"]
["","Oro srauto greitis","Šildymas","Vidutinis","m³/min.","9","9"]
["","","Šildymas","Mažas","m³/min.","5.5","5.5"]
["","","","Tylus veikimas","m³/min.","4.4","4.4"]
["Garso galingumo lygis","Vėsinimas","","","dBA","58","58"]
["","Šildymas","","","dBA","58","58"]
["Garso slėgio lygis","Aušinimas","","Aukštas","dBA","43","43"]
["","Vėsinimas","","Vidutinis","dBA","35","35"]
["","","","Žemas","dBA","26","26"]
["","","","Tylus veikimas","dBA","21","21"]
["","Šildymas","","Aukštas","dBA","43","43"]
["","","","Vidutinis","dBA","35","35"]
["","","","Žemas","dBA","26","26"]
["","","","Tylus veikimas","dBA","21","21"]
["Aušinimo medžiaga","GWP","","","","675","675"]
["Vamzdžių jungtys","Skystis","","OD","mm","6.35","6.35"]
["","Dujos","","Iš. diam.","mm","9.5","9.5"]
["","Drenažas","","","","18","18"]
["Valdymo sistemos","Infrared remote control","","","","ARC480A53","ARC480A53"]
["Valdymo sistemos","Laidinis nuotolinio valdymo pultelis","","","","BRC073A1","BRC073A1"]
["Standartiniai priedai","Installation manual","","","","1","1"]
["","Wireless remote control","","","","1","1"]
["","AAA dry-cell batteries","","","","2","2"]
["","General safety precautions","","","","1","1"]
["","Operation manual","","","","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1"]
["","Silver particle filter","","","","1","1"]
["","Remote control holder","","","","1","1"]
["","Screw bag","","","","1","1"]
["El. tiekimas","Fazė","","","","1~","1~"]
["Maitinimas","Dažnis","","","Hz","50","50"]
["","Įtampa","","","V","220-240","220-240"]