{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":8,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXZ-N"]
[]
[]
[]
[]
["","","","","","FTXZ25NV1B","FTXZ35NV1B","FTXZ50NV1B"]
["Garso slėgio lygis","Šildymas","","Aukštas","dBA","39","42","44"]
["","","","Tylus veikimas","dBA","19","19","24"]
["","","","Žemas","dBA","28","29","31"]
["","Aušinimas","","Tylus veikimas","dBA","19","19","23"]
["","","","Žemas","dBA","26","27","30"]
["","","","Aukštas","dBA","38","42","47"]
["","","","Nom.","dBA","35","36","38"]
["","Aušinimas","","Nom.","dBA","33","35","38"]
["Standartiniai priedai","Fotokatalizinis oro gryninimo ir kvapų šalinimo filtras","","","","1","1","1"]
["","Belaidis nuotolinis valdymas","","","","1","1","1"]
["","Sausosios baterijos","","","","2","2","2"]
["","Nuotolinio valdymo pulto laikiklis","","","","1","1","1"]
["","Vidinės įrangos pritvirtinimo varžtai","","","","3","3","3"]
["","Pritvirtinimo plokštė","","","","1","1","1"]
["Valdymo sistemos","Infrared remote control","","","","ARC477A1","ARC477A1","ARC477A1"]
["Vamzdžių jungtys","Skystis","","OD","mm","6.35","6.35","6.35"]
["","Dujos","","Iš. diam.","mm","9.5","9.5","9.5"]
["Tiekiama galia","Aušinimas","","Nom.","kW","0.030","0.030","0.030"]
["","Šildymas","","Nom.","kW","0.030","0.030","0.030"]
["Triukšmingumo lygis","Vėsinimas","","","dBA","54","57","60"]
["","Šildymas","","","dBA","56","57","59"]
["Matmenys","Įrenginys","","Plotis","mm","798","798","798"]
["","","","Gylis","mm","372","372","372"]
["","","","Aukštis","mm","295","295","295"]
["Korpusas","Spalva","","","","Balta spalva","Balta spalva","Balta spalva"]
["Svoris","Įrenginys","","","kg","15","15","15"]
["Ventiliatorius","Oro srauto koef.","Šildymas","Didelis","m³/min.","11.7","13.3","14.4"]
["","","","Mažas","m³/min.","6.7","6.9","7.7"]
["","","","Tylus veikimas","m³/min.","4.8","4.8","5.9"]
["","","Vėsinimas","Mažas","m³/min.","5.3","5.6","6.6"]
["","","","Didelis","m³/min.","10.7","12.1","15.0"]
["","","","Tylus veikimas","m³/min.","4.0","4.0","4.6"]
["","","","Nom.","m³/min.","8.6","9.2","10.7"]
["","","Vėsinimas","Nom.","m³/min.","7.5","8.4","9.2"]
["Power supply","Fazė","","","","1~","1~","1~"]
["","Pavadinimas","","","","V1","V1","V1"]
["","Dažnis","","","Hz","50","50","50"]
["","Įtampa","","","V","220-240","220-240","220-240"]
["Pastabos","","","","","(1) - 220 V","(1) - 220 V","(1) - 220 V"]
["","","","","","(2) - 230 V","(2) - 230 V","(2) - 230 V"]
["","","","","","(3) - 240 V","(3) - 240 V","(3) - 240 V"]
["","","","","","(4) - Šilumokaičio priekis","(4) - Šilumokaičio priekis","(4) - Šilumokaičio priekis"]
["","","","","","(5) - Šilumokaičio galas","(5) - Šilumokaičio galas","(5) - Šilumokaičio galas"]