{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":16,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUA-A / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FUA100AVEB / RZQG100L8Y1B","FUA125AVEB / RZQG125L8Y1B","FUA71AVEB / FUA71AVEB / RZQG100L8Y1B","FUA71AVEB / FUA71AVEB / RZQG125L8Y1B","FUA100AVEB9 / RZQG100L8Y1B","FUA125AVEB9 / RZQG125L8Y1B","FUA71AVEB9 / FUA71AVEB9 / RZQG100L8Y1B","FUA71AVEB9 / FUA71AVEB9 / RZQG125L8Y1B","FUA100AVEB / RZQG71L8Y1B","FUA100AVEB9 / RZQG71L8Y1B","FUA71AVEB / RZQG71L8Y1B","FUA71AVEB9 / RZQG71L8Y1B"]
["Energijos naudojimo efektyvumo klasė","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Aušinimo galingumas","Nom.","","kW","","","","","","","","","6.80","6.80","6.80","6.80"]
["Patalpos vėsinimas","SEER","","","","","","","","","","","6.42","6.42","6.42","6.42"]
["","Metinės energijos sąnaudos","","kWh/a","","","","","","","","","371","371","371","371"]
["","Vėsinimas","Pdesign","kW","","","","","","","","","6.80","6.80","6.80","6.80"]
["","Energijos efektyvumo klasė","","","","","","","","","","","A++","A++","A++","A++"]
["Patalpos šildymas (vidutinis klimatas)","Pajėgumas","Pdesign","kW","","","","","","","","","7.60","7.60","7.60","7.60"]
["","SCOP/A","","","","","","","","","","","4.20","4.20","4.20","4.20"]
["","Energijos efektyvumo klasė","","","","","","","","","","","A+","A+","A+","A+"]
["","Metinės energijos sąnaudos","","kWh/a","","","","","","","","","2,534","2,534","2,534","2,534"]
["Vardinis našumas","EER","","","","","","","","","","","4.07","4.07","4.07","4.07"]
["Pastabos","","","","","","","","","","","","(1) - Žr. specialų darbinio diapazono brėžinį","(1) - Žr. specialų darbinio diapazono brėžinį","(1) - Nominalus aušinimo galingumas yra pagrįstas: patalpų temperatūra: 27°CDB/19°CWB, išorinė temperatūra: 35 °CDB, ekvivalentinis šaltnešio vamzdynas: 5 m, aukščio skirtumas: 0 m.","(1) - Nominalus aušinimo galingumas yra pagrįstas: patalpų temperatūra: 27°CDB/19°CWB, išorinė temperatūra: 35 °CDB, ekvivalentinis šaltnešio vamzdynas: 5 m, aukščio skirtumas: 0 m."]
["","","","","","","","","","","","","(2) - Žr. atskirą elektros duomenų brėžinį","(2) - Žr. atskirą elektros duomenų brėžinį","(2) - Nominali šildymo galia nustatyta remiantis: vidaus temperatūra: 20 °CDB, lauko temperatūra: 7 °CDB, 6 °CWB, ekvivalentinis aušinimo medžiagos vamzdyno ilgis: 5 m, aukščių skirtumas: 0 m.","(2) - Nominali šildymo galia nustatyta remiantis: vidaus temperatūra: 20 °CDB, lauko temperatūra: 7 °CDB, 6 °CWB, ekvivalentinis aušinimo medžiagos vamzdyno ilgis: 5 m, aukščių skirtumas: 0 m."]
["Vardinis našumas","Metinis energijos sunaudojimas","","kWh","","","","","","","","","","","835","835"]
["","COP","","","","","","","","","","","","","4.08","4.08"]
["","Energijos suvartojimo ženklinimo direktyva","Vėsinimas","","","","","","","","","","","","A","A"]
["","","Šildymas","","","","","","","","","","","","A","A"]
["Šildymo galingumas","Nom.","","kW","","","","","","","","","","","7.50","7.50"]
["Pastabos","","","","","","","","","","","","","","(3) - Žr. specialų darbinio diapazono brėžinį","(3) - Žr. specialų darbinio diapazono brėžinį"]
["","","","","","","","","","","","","","","(4) - Žr. atskirą elektros duomenų brėžinį","(4) - Žr. atskirą elektros duomenų brėžinį"]