{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":82,"n_cols":11,"rows_kept":82,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUA-A"]
[]
[]
[]
[]
["","","","","","FUA71AVEB9","FUA100AVEB9","FUA125AVEB9","FUA71AVEB (Archived)","FUA100AVEB (Archived)","FUA125AVEB (Archived)"]
["Garso slėgio lygis","Šildymas","","Aukštas","dBA","","","","41","46","47"]
["","","","Vidutinis","dBA","","","","38","42","43"]
["","","","Žemas","dBA","","","","35","39","40"]
["","Aušinimas","","Vidutinis","dBA","","","","38","42","43"]
["","","","Žemas","dBA","","","","35","39","40"]
["","","","Aukštas","dBA","","","","41","46","47"]
["Standartiniai priedai","Eksploatavimo vadovas","","","","","","","1","1","1"]
["","Įrengimo vadovas","","","","","","","1","1","1"]
["","Drenavimo žarna","","","","","","","1","1","1"]
["","Šilumos izoliacinis vamzdis","","","","","","","3","3","3"]
["","Sujungimų apvyniojimai","","","","","","","10","10","10"]
["","Žarnos juosta","","","","","","","1","1","1"]
["","Sandarinimo medžiaga","","","","","","","4","4","4"]
["","Poveržlę fiksuojanti plokštė","","","","","","","1","1","1"]
["","Drenavimo jungtis","","","","","","","1","1","1"]
["","Neaustinė medžiaga","","","","","","","1","1","1"]
["","Poveržlė","","","","","","","8","8","8"]
["","Tvirtinimo varžtas drenažo žarnai","","","","","","","5","5","5"]
["Valdymo sistemos","Wired remote control","","","","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Vėsinimo pajėgumas","Bendras pajėgumas","","Nom.","kW","","","","","","12.1"]
["Piping connections","Skysčių vamzdis","","OD","mm","","","","9.52","9.52","9.52"]
["","Dujos","","Iš. diam.","mm","","","","15.9","15.9","15.9"]
["","Drenažo vamzdis","","","","","","","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)"]
["Garso galingumo lygis","Vėsinimas","","","dBA","","","","59","64","65"]
["","Šildymas","","","dBA","","","","59","64"]
["Matmenys","Vienetas","","Plotis","mm","","","","950","950","950"]
["","","","Gylis","mm","","","","950","950","950"]
["","","","Aukštis","mm","","","","198","198","198"]
["Korpusas","Medžiaga","","","","","","","Derva","Derva","Derva"]
["","Colour","","","","","","","Ryškiai balta","Ryškiai balta","Ryškiai balta"]
["Svoris","Įrenginys","","","kg","","","","25.0","26.0","26"]
["Ventiliatorius","Oro debitas","Šildymas","Didelis","m³/min.","","","","23.0","31.0","32.5"]
["","","","Vidutinis","m³/min.","","","","19.5","25.5","26.5"]
["","","","Mažas","m³/min.","","","","16.0","20.0","20.5"]
["","","Vėsinimas","Mažas","m³/min.","","","","16.0","20.0","20.5"]
["","","","Vidutinis","m³/min.","","","","19.5","25.5","26.5"]
["","","","Didelis","m³/min.","","","","23.0","31.0","32.5"]
["Drenavimo aukštis","mm","","","","","","","600","600","600"]
["Šildymo galingumas","Bendras pajėgumas","","Nom.","kW","","","","","","13.5"]
["Korpusas","Spalva","","","","Ryškiai balta","Ryškiai balta","Ryškiai balta"]
["","Medžiaga","","","","Derva","Derva","Derva"]
["Matmenys","Įrenginys","","Aukštis","mm","198","198","198"]
["","","","Plotis","mm","950","950","950"]
["","","","Gylis","mm","950","950","950"]
["Svoris","Įrenginys","","","kg","25.0","26.0","26.0"]
["Ventiliatorius","Oro debitas","Aušinimas","Didelis","m³/min.","23.0","31.0","32.5"]
["","Oro srauto greitis","Vėsinimas","Vidutinis","m³/min.","19.5","25.5","26.5"]
["","","","Mažas","m³/min.","16.0","20.0","20.5"]
["","","Šildymas","Didelis","m³/min.","23.0","31.0","32.5"]
["","Oro srauto greitis","Šildymas","Vidutinis","m³/min.","19.5","25.5","26.5"]
["","","Šildymas","Mažas","m³/min.","16.0","20.0","20.5"]
["Garso galingumo lygis","Vėsinimas","","","dBA","59","64","65"]
["Garso slėgio lygis","Aušinimas","","Aukštas","dBA","41","46","47"]
["","Vėsinimas","","Vidutinis","dBA","38","42","43"]
["","","","Žemas","dBA","35","39","40"]
["","Šildymas","","Aukštas","dBA","41","46","47"]
["","","","Vidutinis","dBA","38","42","43"]
["","","","Žemas","dBA","35","39","40"]
["Vamzdžių jungtys","Skystis","","OD","mm","9.52","9.52","9.52"]
["","Dujos","","Iš. diam.","mm","15.9","15.9","15.9"]
["","Drenažas","","","","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)"]
["Drenavimo aukštis","mm","","","","600","600","600"]
["Standartiniai priedai","Installation manual","","","","1","1","1"]
["","Thermal insulation tube","","","","3","3","3"]
["","Non woven fabric","","","","1","1","1"]
["","Drain joint","","","","1","1","1"]
["","Hose band","","","","1","1","1"]
["","Operation manual","","","","1","1","1"]
["","Drain hose","","","","1","1","1"]
["","Fixing screw for drain hose","","","","5","5","5"]
["","Sealing material","","","","4","4","4"]
["","Tie-wraps","","","","10","10","10"]
["","Washer","","","","8","8","8"]
["","Washer fixing plate","","","","1","1","1"]
["Aušinimo galingumas","Bendras galingumas","","Nom.","kW","","","12.10"]
["Šildymo galia","Bendras pajėgumas","","Nom.","kW","","","13.5"]