{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":45,"n_cols":7,"rows_kept":45,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUQ-C"]
[]
[]
[]
[]
["","","","","FUQ71CVEB","FUQ100CVEB","FUQ125CVEB"]
["Garso slėgio lygis","Šildymas","Aukštas","dBA","41","46","47"]
["","","Nom.","dBA","38","42","43"]
["","","Žemas","dBA","35","39","40"]
["","Aušinimas","Žemas","dBA","35","39","40"]
["","","Aukštas","dBA","41","46","47"]
["","","Nom.","dBA","38","42","43"]
["Standartiniai priedai","Įrengimo vadovas","","","Įrengimo vadovas","Įrengimo vadovas","Įrengimo vadovas"]
["","Eksploatavimo vadovas","","","Eksploatavimo vadovas","Eksploatavimo vadovas","Eksploatavimo vadovas"]
["","Atitikties deklaracija","","","Atitikties deklaracija","Atitikties deklaracija","Atitikties deklaracija"]
["","Drenavimo žarna","","","Drenavimo žarna","Drenavimo žarna","Drenavimo žarna"]
["","Metalinis veržtuvas","","","Metalinis veržtuvas","Metalinis veržtuvas","Metalinis veržtuvas"]
["","Poveržlė kablio laikytuvui","","","Poveržlė kablio laikytuvui","Poveržlė kablio laikytuvui","Poveržlė kablio laikytuvui"]
["","Veržtuvai","","","Veržtuvai","Veržtuvai","Veržtuvai"]
["","Poveržlės spaustukas","","","Poveržlės spaustukas","Poveržlės spaustukas","Poveržlės spaustukas"]
["","Jungčių izoliacinė ir sandarinimo medžiaga","","","Jungčių izoliacinė ir sandarinimo medžiaga","Jungčių izoliacinė ir sandarinimo medžiaga","Jungčių izoliacinė ir sandarinimo medžiaga"]
["","Alkūnė","","","Alkūnė","Alkūnė","Alkūnė"]
["","Montavimo būdas","","","Montavimo būdas","Montavimo būdas","Montavimo būdas"]
["","Blokavimo medžiaga","","","Blokavimo medžiaga","Blokavimo medžiaga","Blokavimo medžiaga"]
["","L formos vamzdis","","","L formos vamzdis","L formos vamzdis","L formos vamzdis"]
["","Varžtai","","","Varžtai","Varžtai","Varžtai"]
["","Neaustinė medžiaga","","","Neaustinė medžiaga","Neaustinė medžiaga","Neaustinė medžiaga"]
["Kontrolės sistemos","Wired remote control","","","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B"]
["","Infrared remote control","","","BRC7C58","BRC7C58","BRC7C58"]
["Vamzdžių jungtys","Skystis","OD","mm","9.52","9.52","9.52"]
["","Dujos","Iš. diam.","mm","15.9","15.9","15.9"]
["","Drenažo vamzdis","","","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)"]
["Sound power level","Vėsinimas","","dBA","59","64","65"]
["","Šildymas","","dBA","59","64","65"]
["Matmenys","Įrenginys","Plotis","mm","950","950","950"]
["","","Gylis","mm","950","950","950"]
["","","Aukštis","mm","198","198","198"]
["Korpusas","Medžiaga","","","Derva","Derva","Derva"]
["","Spalva","","","Ryškiai balta","Ryškiai balta","Ryškiai balta"]
["Svoris","Įrenginys","","kg","25","26","26"]
["Drenavimo aukštis","mm","","","600","600","600"]
["Power supply","Fazė","","","1~","1~","1~"]
["","Dažnis","","Hz","50/60","50/60","50/60"]
["","Pavadinimas","","","VE","VE","VE"]
["","Įtampa","","V","220-240/220","220-240/220","220-240/220"]