{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":11,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVQ-C / RZQG-L9V1"]
[]
[]
[]
[]
["","","","","FVQ100CVEB / RZQG71L9V1B","FVQ71CVEB / RZQG71L9V1B","FVQ100CVEB / RZQG100L9V1B","FVQ140CVEB / RZQG100L9V1B","FVQ125CVEB / RZQG125L9V1B","FVQ140CVEB / RZQG125L9V1B","FVQ140CVEB / RZQG140L9V1B"]
["Aušinimo galingumas","Nom.","","kW","","6.8","9.5","","12.0","","13.4"]
["Patalpos vėsinimas","SEER","","","6.31","6.23","5.61","5.61","5.61","5.61"]
["","Metinės energijos sąnaudos","","kWh/a","378","383","593","593","749","749"]
["","Vėsinimas","Pdesign","kW","6.80","6.80","9.50","9.50","12.00","12.00"]
["","Energijos efektyvumo klasė","","","A++","A++","A+","A+","A+","A+"]
["Patalpos šildymas (vidutinis klimatas)","Pajėgumas","Pdesign","kW","6.33","6.33","11.30","11.30","11.30","11.30"]
["","SCOP/A","","","4.05","4.05","4.20","4.20","3.87","3.87"]
["","Energijos efektyvumo klasė","","","A+","A+","A+","A+","A","A"]
["","Metinės energijos sąnaudos","","kWh/a","2,189","2,189","3,767","3,767","4,088","4,088"]
["Vardinis našumas","Metinis energijos sunaudojimas","","kWh","","1,010","1,245","","1,870","","2,085"]
["","EER","","","","3.37","3.81","","3.21","","3.21"]
["","COP","","","","3.64","4.14","","3.70","","3.61"]
["","Energijos suvartojimo ženklinimo direktyva","Vėsinimas","","","A","A","","A"]
["","","Šildymas","","","A","A","","A"]
["Šildymo galingumas","Nom.","","kW","","7.5","10.8","","13.5","","15.5"]
["Pastabos","","","","","(1) - Metinės energijos sąnaudos pagal energijos žymėjimo direktyvą 2002/31/EB","(1) - EER/COP pagal „Eurovent 2012“, skirta naudoti tik už ES ribų","","(1) - EER/COP pagal „Eurovent 2012“, skirta naudoti tik už ES ribų","","(1) - EER/COP pagal „Eurovent 2012“, skirta naudoti tik už ES ribų"]
["","","","","","(2) - SEER ir SCOP pagal EN 14825","(2) - Nominalus efektyvumas: vėsinimas esant 35°/27° nominaliąja apkrova, šildymas esant 7°/20° nominaliąja apkrova","","(2) - Nominalus efektyvumas: vėsinimas esant 35°/27° nominaliąja apkrova, šildymas esant 7°/20° nominaliąja apkrova","","(2) - Nominalus efektyvumas: vėsinimas esant 35°/27° nominaliąja apkrova, šildymas esant 7°/20° nominaliąja apkrova"]