{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":7,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXG-K / RXG-L"]
[]
[]
[]
[]
["","","","","FVXG25K2V1B / RXG25L2V1B","FVXG35K2V1B / RXG35L2V1B","FVXG50K2V1B / RXG50L2V1B"]
["Aušinimo galingumas","Min.","","kW","1.3","1.4","1.7"]
["","Nom.","","kW","2.5","3.5","5.0"]
["","Maks.","","kW","3.0","3.8","5.6"]
["Šildymo galingumas","Min.","","kW","1.3","1.4","1.7"]
["","Nom.","","kW","3.4","4.5","5.8"]
["","Maks.","","kW","4.5","5.0","8.1"]
["Nominalus efektyvumas","EER","","","4.63","3.72","3.31"]
["","COP","","","4.42","3.75","3.69"]
["","Metinis energijos sunaudojimas","","kWh","270","470","755"]
["Vardinis našumas","Energijos suvartojimo ženklinimo direktyva","Vėsinimas","","A","A","A"]
["","","Šildymas","","A","A","A"]
["Vamzdžių jungtys","Dujos","Iš. diam.","mm","9.5","9.5","12.7"]
["","Skystis","OD","mm","6.35","6.35","6.35"]
["Patalpos vėsinimas","Energijos efektyvumo klasė","","","A++","A++","A"]
["","Vėsinimas","Pdesign","kW","2.50","3.50","5.00"]
["","SEER","","","6.53","6.48","5.41"]
["","Metinės energijos sąnaudos","","kWh/a","134","189","324"]
["Patalpos šildymas (vidutinis klimatas)","Energijos efektyvumo klasė","","","A++","A+","A+"]
["","Pajėgumas","Pdesign","kW","2.80","3.10","4.60"]
["","SCOP/A","","","4.65","4.00","4.18"]
["","Metinės energijos sąnaudos","","kWh/a","842","1087","1543"]
["Pastabos","","","","(1) - Vėsinimas: vidinė temp. 27 °CDB, 19 °CWB; lauko temp. 35 °CDB, 24 °CWB","(1) - Vėsinimas: vidinė temp. 27 °CDB, 19 °CWB; lauko temp. 35 °CDB, 24 °CWB","(1) - Vėsinimas: vidinė temp. 27 °CDB, 19 °CWB; lauko temp. 35 °CDB, 24 °CWB"]
["","","","","(2) - Šildymas: vidaus temp. 20 °CDB; lauko temp. 7 °CDB, 6 °CWB","(2) - Šildymas: vidaus temp. 20 °CDB; lauko temp. 7 °CDB, 6 °CWB","(2) - Šildymas: vidaus temp. 20 °CDB; lauko temp. 7 °CDB, 6 °CWB"]