{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":8,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXM-A9"]
[]
[]
[]
[]
["","","","","","FVXM25A3V1B9","FVXM35A3V1B9","FVXM50A3V1B9"]
["Tiekiama galia","Aušinimas","","Nom.","kW","0.02","0.02","0.03"]
["","Šildymas","","Nom.","kW","0.02","0.03","0.03"]
["Korpusas","Spalva","","","","Balta","Balta","Balta"]
["Matmenys","Įrenginys","","Aukštis","mm","600","600","600"]
["","","","Plotis","mm","750","750","750"]
["","","","Gylis","mm","238","238","238"]
["Svoris","Įrenginys","","","kg","17","17","17"]
["Ventiliatorius","Oro debitas","Aušinimas","Didelis","m³/min.","8.7","9.2","11.6"]
["","Oro srauto greitis","Vėsinimas","Vidutinis","m³/min.","7","7","9"]
["","","","Mažas","m³/min.","4.9","4.9","6.6"]
["","","","Tylus veikimas","m³/min.","4.1","4.1","5.4"]
["","","Šildymas","Didelis","m³/min.","9.2","9.8","12.8"]
["","Oro srauto greitis","Šildymas","Vidutinis","m³/min.","7.2","7.2","10"]
["","","Šildymas","Mažas","m³/min.","5.6","5.6","8.4"]
["","","","Tylus veikimas","m³/min.","4.1","4.1","5.9"]
["Garso galingumo lygis","Vėsinimas","","","dBA","52","53","61"]
["","Šildymas","","","dBA","52","53","62"]
["Garso slėgio lygis","Aušinimas","","Aukštas","dBA","38","39","44"]
["","Vėsinimas","","Vidutinis","dBA","32","32","38"]
["","","","Žemas","dBA","25","25","31"]
["","","","Tylus veikimas","dBA","20","20","27"]
["","Šildymas","","Aukštas","dBA","38","39","46"]
["","","","Vidutinis","dBA","32","32","40"]
["","","","Žemas","dBA","25","25","35"]
["","","","Tylus veikimas","dBA","19","19","29"]
["Aušinimo medžiaga","GWP","","","","675","675","675"]
["Vamzdžių jungtys","Skystis","","OD","mm","6.4","6.4","6.4"]
["","Dujos","","Iš. diam.","mm","9.5","9.5","12.7"]
["","Drenažas","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Valdymo sistemos","Nuotolinis infraraudonųjų spindulių pultelis","","","","ARC466A66","ARC466A66","ARC466A66"]
["","Laidinis nuotolinio valdymo pultelis","","","","BRC073A1","BRC073A1","BRC073A1"]
["Standartiniai priedai","Installation manual","","","","1","1","1"]
["","Wireless remote control","","","","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2"]
["","General safety precautions","","","","1","1","1"]
["","Operation manual","","","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2","2"]
["","Remote control holder","","","","1","1","1"]
["","Screw bag","","","","1","1","1"]
["El. tiekimas","Fazė","","","","1~","1~","1~"]
["Maitinimas","Dažnis","","","Hz","50","50","50"]
["","Įtampa","","","V","220-240","220-240","220-240"]