{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":6,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXTM-A"]
[]
[]
[]
[]
["","","","","","FVXTM30A3V1B"]
["Tiekiama galia","Aušinimas","","Nom.","kW","0.02"]
["","Šildymas","","Nom.","kW","0.03"]
["Korpusas","Spalva","","","","Balta"]
["Matmenys","Įrenginys","","Aukštis","mm","600"]
["","","","Plotis","mm","750"]
["","","","Gylis","mm","238"]
["Svoris","Įrenginys","","","kg","17"]
["Ventiliatorius","Oro debitas","Aušinimas","Didelis","m³/min.","9"]
["","Oro srauto greitis","Vėsinimas","Vidutinis","m³/min.","6.7"]
["","","","Mažas","m³/min.","4.8"]
["","","","Tylus veikimas","m³/min.","4"]
["","","Šildymas","Didelis","m³/min.","9.4"]
["","Oro srauto greitis","Šildymas","Vidutinis","m³/min.","6.8"]
["","","Šildymas","Mažas","m³/min.","5.3"]
["","","","Tylus veikimas","m³/min.","4"]
["Garso galingumo lygis","Vėsinimas","","","dBA","53"]
["","Šildymas","","","dBA","53"]
["Garso slėgio lygis","Aušinimas","","Aukštas","dBA","39"]
["","Vėsinimas","","Vidutinis","dBA","32"]
["","","","Žemas","dBA","25"]
["","","","Tylus veikimas","dBA","20"]
["","Šildymas","","Aukštas","dBA","39"]
["","","","Vidutinis","dBA","32"]
["","","","Žemas","dBA","25"]
["","","","Tylus veikimas","dBA","19"]
["Aušinimo medžiaga","GWP","","","","675"]
["Vamzdžių jungtys","Skystis","","OD","mm","6.35"]
["","Dujos","","Iš. diam.","mm","9.5"]
["","Drenažas","","","","VP20 (I.D. 20/O.D. 26)"]
["Control systems","Infrared remote control","","","","ARC466A66"]
["Valdymo sistemos","Laidinis nuotolinio valdymo pultelis","","","","BRC073A1"]
["Standartiniai priedai","Installation manual","","","","1"]
["","Wireless remote control","","","","1"]
["","AAA dry-cell batteries","","","","2"]
["","General safety precautions","","","","1"]
["","Operation manual","","","","1"]
["","Titanium apatite deodorizing filter","","","","2"]
["","Remote control holder","","","","1"]
["","Screw bag","","","","2"]
["El. tiekimas","Fazė","","","","1~"]
["Maitinimas","Dažnis","","","Hz","50"]
["","Įtampa","","","V","220-240"]