{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":63,"n_cols":6,"rows_kept":63,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MCK55W"]
[]
[]
[]
[]
["","","","","","MCK55WVM"]
["Tipas","","","","","Drėkinamasis oro valymo įtaisas"]
["Panaudojimas","","","","","Statomas ant grindų"]
["Korpusas","Spalva","","","","Balta"]
["Matmenys","Įrenginys","","Aukštis","mm","700"]
["","","","Plotis","mm","270"]
["","","","Gylis","mm","270"]
["Svoris","Įrenginys","","","kg","9.5"]
["Naudojamas patalpos plotas","m²","","","","41 (1), 82 (2)"]
["CADR","m³/val.","","","","320"]
["Oro valymas","Tiekiama galia","","Turbo","kW","0.056"]
["","","","M","kW","0.017"]
["","","","L","kW","0.010"]
["","","","Tylus","kW","0.007"]
["Drėkinimas","Tiekiama galia","","Turbo","kW","0.058"]
["","","","M","kW","0.019"]
["","","","L","kW","0.014"]
["","","","Tylus","kW","0.011"]
["","Vandens bako talpa","","","l","2.7"]
["Garso slėgio lygis","Oro valymas","","Turbo","dBA","53.0"]
["","","","Vidutinis","dBA","39.0"]
["","","","Žemas","dBA","29.0"]
["","","","Tylus","dBA","19.0"]
["","Drėkinimas","","Turbo","dBA","53.0"]
["","","","Vidutinis","dBA","39.0"]
["","","","Žemas","dBA","33.0"]
["","","","Tylus","dBA","25.0"]
["Ventiliatorius","Oro debitas","Oro valymas","Turbo","m³/val.","330"]
["","","","Vidutinis","m³/val.","192"]
["","","","Mažas","m³/val.","120"]
["","","","Tylus","m³/val.","54"]
["","","Drėkinimas","Turbo","m³/val.","330"]
["","","","Vidutinis","m³/val.","192"]
["","","","Mažas","m³/val.","144"]
["","","","Tylus","m³/val.","102"]
["Dulkių surinkimo būdas","","","","","Elektrostatinis HEPA filtras"]
["Blogų kvapų pašalinimo būdas","","","","","„Flash streamer“ + kvapus pašalinantis katalizatorius"]
["Standartiniai priedai","Operation manual","","","","1"]
["","Electrostatic HEPA filter","","","","1"]
["","Deodorising filter","","","","1"]
["","Caster","","","","4"]
["","Humidifying filter","","","","2"]
["","Remote control holder","","","","1"]
["","Remote control lid","","","","1"]
["Maitinimo kabelis","Maitinimo kabelis","","","","1.8"]
["El. tiekimas","Fazė","","","","1~"]
["Maitinimas","Maitinimas-=-Dažnis","","Dažnis","","50/60"]
["","Maitinimas-=-Įtampa","","Įtampa","","220-240/220-230"]
["Darbinė srovė","Oro valymas","Darbinė srovė-=-Oro valymas-=-Turbo","Turbo","","0.50"]
["","","Darbinė srovė-=-Oro valymas-=-Vidutinis","Vidutinis","","0.19"]
["","","Darbinė srovė-=-Oro valymas-=-Žema","Žema","","0.12"]
["","","Darbinė srovė-=-Oro valymas-=-Tylus","Tylus","","0.09"]
["","Drėkinimas","Darbinė srovė-=-Drėkinimas-=-Turbo","Turbo","","0.50"]
["","","Darbinė srovė-=-Drėkinimas-=-Vidutinis","Vidutinis","","0.20"]
["","","Darbinė srovė-=-Drėkinimas-=-Žema","Žema","","0.15"]
["","","Darbinė srovė-=-Drėkinimas-=-Tylus","Tylus","","0.13"]
["Pastabos","","","","","(1) - Darbinės patalpos sritis yra pritaikyta naudoti įrenginį didžiausiu ventiliatoriaus greičiu (HH). Darbinis patalpos sritis nurodo plotą, iš kurio per 30 minučių gali būti pašalintas tam tikras dulkių dalelių kiekis. (JEM 1467)"]
["","","","","","(2) - Konvertuota iš testinių reikšmių į NRCC standartus pagal JEM1467."]