{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":54,"n_cols":6,"rows_kept":54,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MCK70YV"]
[]
[]
[]
[]
["","","","","","MCK70YVM"]
["Tipas","","","","","Drėkinamasis oro valymo įtaisas"]
["Panaudojimas","","","","","Statomas ant grindų"]
["Korpusas","Spalva","","","","Baltas (N9. 0)"]
["Matmenys","Įrenginys","","Aukštis","mm","600 (5)"]
["","","","Plotis","mm","395"]
["","","","Gylis","mm","287"]
["Svoris","Įrenginys","","","kg","12.5"]
["Naudojamas patalpos plotas","m²","","","","48 (1), 96 (2)"]
["CADR","m³/val.","","","","375"]
["Oro valymas","Tiekiama galia","","Turbo","kW","0.066"]
["","","","M","kW","0.016"]
["","","","L","kW","0.01"]
["","","","Tylus","kW","0.008"]
["Drėkinimas","Tiekiama galia","","Turbo","kW","0.068"]
["","","","M","kW","0.018"]
["","","","L","kW","0.012"]
["","","","Tylus","kW","0.011"]
["","Vandens bako talpa","","","l","3.6"]
["Garso slėgio lygis","Oro valymas","","Turbo","dBA","54"]
["","","","Vidutinis","dBA","37"]
["","","","Žemas","dBA","27"]
["","","","Tylus","dBA","18"]
["","Drėkinimas","","Turbo","dBA","54"]
["","","","Vidutinis","dBA","37"]
["","","","Žemas","dBA","27"]
["","","","Tylus","dBA","23"]
["Ventiliatorius","Oro debitas","Oro valymas","Turbo","m³/val.","420"]
["","","","Vidutinis","m³/val.","210"]
["","","","Mažas","m³/val.","132"]
["","","","Tylus","m³/val.","60"]
["","","Drėkinimas","Turbo","m³/val.","420"]
["","","","Vidutinis","m³/val.","210"]
["","","","Mažas","m³/val.","132"]
["","","","Tylus","m³/val.","102"]
["Dulkių surinkimo būdas","","","","","Elektrostatinis HEPA filtras"]
["Blogų kvapų pašalinimo būdas","","","","","„Flash streamer“ + kvapus pašalinantis katalizatorius"]
["Standartiniai priedai","Operation manual","","","","1"]
["","Electrostatic HEPA filter","","","","1"]
["","Deodorising filter","","","","1"]
["","Caster","","","","4"]
["","Humidifying filter","","","","1"]
["Maitinimo kabelis","m","","","","2"]
["El. tiekimas","Fazė","","","","1~"]
["Maitinimas","Dažnis","","","Hz","50/60"]
["","Įtampa","","","V","220-240/220-230"]
["Pastabos","","","","","(1) - Tinkama apimties sritis, naudojant įrenginį didžiausiu ventiliatoriaus greičiu (HH). Apimties sritis nurodo plotą, iš kurio per 30 minučių gali būti pašalintas tam tikras dulkių dalelių kiekis."]
["","","","","","(2) - Konvertuota iš testinių reikšmių į NRCC standartus pagal JEM1467."]
["","","","","","(3) - Darbinio triukšmo lygiai – vidutinės reikšmės, matuojamos 1 m atstumu nuo įrenginio priekio, kairės, dešinės ir viršaus. (Jos yra lygios beaidėje patalpoje išmatuotoms reikšmėms)"]