{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":39,"n_cols":20,"rows_kept":39,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RX-K"]
[]
[]
[]
[]
["","","","","","RX20K2V1B","RX20K5V1B","RX20K5V1B9","RX25K2V1B","RX25K5V1B","RX25K5V1B9","RX35K2V1B","RX35K5V1B","RX35K5V1B9","RX50KV1B","RX50K2V1B","RX60KV1B","RX60K2V1B","RX71KV1B","RX71K2V1B"]
["Ventiliatorius","Oro debitas","Vėsinimas","Labai lėtai","m³/min.","","","","","","","","","","51.3"]
["","","Šildymas","Labai lėtai","m³/min.","","","","","","","","","","51.3"]
["","","","Labai lėtai","cfm","","","","","","","","","","1812"]
["","","Šildymas","Labai lėtai","cfm","","","","","","","","","","1812"]
["Matmenys","Įrenginys","","Aukštis","mm","550","550","550","550","550","550","550","550","550","735","734","735","734","735","734"]
["","","","Plotis","mm","658","658","658","658","658","658","658","658","658","870","870","870","870","870","870"]
["","","","Gylis","mm","275","275","275","275","275","275","275","275","275","320","373","320","373","320","373"]
["Svoris","Įrenginys","","","kg","28","28","28","28","28","28","28","28","28","44","46.0","49","49.0","49","49.0"]
["Kompresorius","Tipas","","","","Hermetiškai užsandarintas stūmoklinis kompresorius","Hermetiškai užsandarintas stūmoklinis kompresorius","Hermetiškai užsandarintas stūmoklinis kompresorius","Hermetiškai užsandarintas stūmoklinis kompresorius","Hermetiškai užsandarintas stūmoklinis kompresorius","Hermetiškai užsandarintas stūmoklinis kompresorius","Hermetiškai užsandarintas stūmoklinis kompresorius","Hermetiškai užsandarintas stūmoklinis kompresorius","Hermetiškai užsandarintas stūmoklinis kompresorius","Hermetiškai užsandarintas stūmoklinis kompresorius","Hermetiškai užsandarintas stūmoklinis kompresorius","Hermetiškai užsandarintas stūmoklinis kompresorius","Hermetiškai užsandarintas stūmoklinis kompresorius","Hermetiškai užsandarintas stūmoklinis kompresorius","Hermetiškai užsandarintas stūmoklinis kompresorius"]
["Veikimo diapazonas","Aušinimas","Aplinkos","Min.","°CDB","-10 (1)","-10 (1)","-10 (1)","-10 (1)","-10 (1)","-10 (1)","-10 (1)","-10 (1)","-10 (1)","-10","","-10"]
["","","","Maks.","°CDB","46","46","46","46","46","46","46","46","46","46","","46"]
["","Šildymas","Aplinkos","Min.","°CWB","-15","-15","-15","-15","-15","-15","-15","-15","-15","-15","","-15"]
["","","","Maks.","°CWB","18","18","18","18","18","18","18","18","18","18","","18"]
["Garso slėgio lygis","Aušinimas","","Aukštas","dBA","46","46","46","46","46","46","48","48","48","47","","49","","52"]
["","","","Nom.","dBA","","","","","","","","","","","47","","49","","52"]
["","Šildymas","","Aukštas","dBA","47","47","47","47","47","47","48","48","48","48","","49","","52"]
["","","","Nom.","dBA","","","","","","","","","","","48","","49","","52"]
["Šaltnešis","Tipas","","","","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A"]
["Aušinimo medžiaga","Užpildytas kiekis","","","kg","0.74","0.74","0.74","0.74","0.74","0.74","1.0","1.0","1.0","1.13","1.13","1.45","1.45","1.45","1.45"]
["Šaltnešis","Užpildas","","","tCO2Eq","1.5","1.5","1.5","1.5","1.5","1.5","2.1","2.1","2.1","2.4","2.36","3.0","3.03","3.0","3.03"]
["Aušinimo medžiaga","GWP","","","","2087.5","2087.5","2087.5","2087.5","2087.5","2087.5","2087.5","2087.5","2087.5","2087.5","2087.5","2087.5","2087.5","2087.5","2087.5"]
["Vamzdžių jungtys","Vamzdžių ilgis","Maks.","OU - IU","m","15","15","15","15","15","15","15","15","15","30","30.0","30","30.0","30","30.0"]
["","Papildoma šaltnešio įkrova","","","kg/m","0,02 (ilgesniems kaip 10m vamzdžiams)","0,02 (ilgesniems kaip 10m vamzdžiams)","0,02 (ilgesniems kaip 10m vamzdžiams)","0,02 (ilgesniems kaip 10m vamzdžiams)","0,02 (ilgesniems kaip 10m vamzdžiams)","0,02 (ilgesniems kaip 10m vamzdžiams)","0,02 (ilgesniems kaip 10m vamzdžiams)","0,02 (ilgesniems kaip 10m vamzdžiams)","0,02 (ilgesniems kaip 10m vamzdžiams)","0,02 (ilgesniems kaip 10m vamzdžiams)","0,02 (ilgesniems kaip 10m vamzdžiams)","0,02 (ilgesniems kaip 10m vamzdžiams)","0,02 (ilgesniems kaip 10m vamzdžiams)","0,02 (ilgesniems kaip 10m vamzdžiams)","0,02 (ilgesniems kaip 10m vamzdžiams)"]
["","Lygio skirtumas","IU - OU","Maks.","m","12","12","12","12","12","12","12","12","12","20","20.0","20","20.0","20","20.0"]
["Standartiniai priedai","Installation manual","","","","1","1","1","1","1","1","1","1","1","1","1","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1","1","1","1","1","1","1","1","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1","1","1","1","1","1","1","1","1","1","1","1"]
["","Drain plug (only heat pump models)","","","","1","1","1","1","1","1","1","1","1","1","1","1","1","1","1"]
["El. tiekimas","Fazė","","","","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~"]
["Maitinimas","Dažnis","","","Hz","50","50","50","50","50","50","50","50","50","50","50","50","50","50","50"]
["","Įtampa","","","V","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]
["Pastabos","","","","","(1) - Darbinis intervalas kartu su FTX-J3: min. 10 °CDB ~ maks. 46 °CDB","(1) - Darbinis intervalas kartu su FTX-J3: min. 10 °CDB ~ maks. 46 °CDB","(1) - Darbinis intervalas kartu su FTX-J3: min. 10 °CDB ~ maks. 46 °CDB","(1) - Darbinis intervalas kartu su FTX-J3: min. 10 °CDB ~ maks. 46 °CDB","(1) - Darbinis intervalas kartu su FTX-J3: min. 10 °CDB ~ maks. 46 °CDB","(1) - Darbinis intervalas kartu su FTX-J3: min. 10 °CDB ~ maks. 46 °CDB","(1) - Darbinis intervalas kartu su FTX-J3: min. 10 °CDB ~ maks. 46 °CDB","(1) - Darbinis intervalas kartu su FTX-J3: min. 10 °CDB ~ maks. 46 °CDB","(1) - Darbinis intervalas kartu su FTX-J3: min. 10 °CDB ~ maks. 46 °CDB"]
["Standartiniai priedai","Drain cap","","","","","","","","","","","","","9","9","9","9","9","9"]