{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":15,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXF-A"]
[]
[]
[]
[]
["","","","","","RXF20A2V1B","RXF20A5V1B","RXF25A2V1B","RXF25A5V1B","RXF35A2V1B","RXF35A5V1B","RXF50A2V1B","RXF60A2V1B","RXF71A2V1B","RXF71A5V1B"]
["Matmenys","Įrenginys","","Aukštis","mm","550","550","550","550","550","550","735","735","734","734"]
["","","","Plotis","mm","658","658","658","658","658","658","825","825","870","870"]
["","","","Gylis","mm","275","275","275","275","275","275","300","300","373","373"]
["Svoris","Įrenginys","","","kg","26","26","26","26","28","28","47","47","50.0","50.0"]
["Compressor","Type","","","","Hermetiškai užsandarintas stūmoklinis kompresorius","Hermetiškai užsandarintas stūmoklinis kompresorius","Hermetiškai užsandarintas stūmoklinis kompresorius","Hermetiškai užsandarintas stūmoklinis kompresorius","Hermetiškai užsandarintas stūmoklinis kompresorius","Hermetiškai užsandarintas stūmoklinis kompresorius","","Hermetiškai užsandarintas stūmoklinis kompresorius","Hermetiškai užsandarintas stūmoklinis kompresorius","Hermetiškai užsandarintas stūmoklinis kompresorius"]
["Veikimo diapazonas","Aušinimas","Aplinkos","Min.","°CDB","-10","-10","-10","-10","-10","-10","-10","-10"]
["","","","Maks.","°CDB","46","46","46","46","46","46","46","46"]
["Garso slėgio lygis","Aušinimas","","Aukštas","dBA","","","","","","","47","49"]
["","","","Nom.","dBA","46","46","46","46","48","48","","","52","52"]
["","Šildymas","","Aukštas","dBA","","","","","","","49","49"]
["","","","Nom.","dBA","47","47","47","47","48","48","","","52","52"]
["Šaltnešis","Tipas","","","","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32"]
["Aušinimo medžiaga","Užpildytas kiekis","","","kg","0.65","0.65","0.65","0.65","0.70","0.70","1.40","1.45","1.15","1.15"]
["Šaltnešis","Užpildas","","","tCO2Eq","0.44","0.44","0.44","0.44","0.48","0.48","0.95","0.98","0.78","0.78"]
["Aušinimo medžiaga","GWP","","","","675.0","675.0","675.0","675.0","675.0","675.0","675.0","675.0","675","675"]
["Vamzdžių jungtys","Vamzdžių ilgis","Maks.","OU - IU","m","15","15","15","15","15","15","30","30","30","30"]
["","Papildoma šaltnešio įkrova","","","kg/m","0,02 (ilgesniems kaip 10m vamzdžiams)","0,02 (ilgesniems kaip 10m vamzdžiams)","0,02 (ilgesniems kaip 10m vamzdžiams)","0,02 (ilgesniems kaip 10m vamzdžiams)","0,02 (ilgesniems kaip 10m vamzdžiams)","0,02 (ilgesniems kaip 10m vamzdžiams)","0,02 (ilgesniems kaip 10m vamzdžiams)","0,02 (ilgesniems kaip 10m vamzdžiams)","0,02 (ilgesniems kaip 10m vamzdžiams)","0,02 (ilgesniems kaip 10m vamzdžiams)"]
["","Lygio skirtumas","IU - OU","Maks.","m","12","12","12","12","12","12","20.0","20.0","20","20"]
["Standartiniai priedai","Installation manual","","","","1","1","1","1","1","1","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1","1","1","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1","1","1","1","1","1","1"]
["","General safety precautions","","","","1","1","1","1","1","1"]
["","Drain plug","","","","1","1","1","1","1","1","1","1","1","1"]
["El. tiekimas","Fazė","","","","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~"]
["Maitinimas","Dažnis","","","Hz","50","50","50","50","50","50","50","50","50","50"]
["","Įtampa","","","V","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]
["Kompresorius","Tipas","","","","","","","","","","Hermetiškai užsandarintas stūmoklinis kompresorius"]
["Standartiniai priedai","Drain cap","","","","","","","","","","","","3","3"]