{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":8,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXF-B"]
[]
[]
[]
[]
["","","","","","RXF20B5V1B","RXF25B5V1B","RXF50B5V1B"]
["Matmenys","Įrenginys","","Aukštis","mm","550","550","734"]
["","","","Plotis","mm","658","658","870"]
["","","","Gylis","mm","275","275","373"]
["Svoris","Įrenginys","","","kg","26","26","46.0"]
["Compressor","Type","","","","","Hermetiškai užsandarintas stūmoklinis kompresorius"]
["Veikimo diapazonas","Aušinimas","Aplinkos","Min.","°C DB","-10","-10"]
["","","","Maks.","°C DB","46","46"]
["Garso slėgio lygis","Aušinimas","","Nom.","dBA","46","46","47"]
["","Šildymas","","Nom.","dBA","47","47","49"]
["Šaltnešis","Tipas","","","","R-32","R-32","R-32"]
["Aušinimo medžiaga","Užpildytas kiekis","","","kg","0.55","0.55","0.90"]
["Šaltnešis","Užpildas","","","tCO2Eq","0.37","0.37","0.61"]
["Aušinimo medžiaga","GWP","","","","675.0","675.0","675"]
["Vamzdžių jungtys","Vamzdžių ilgis","Maks.","OU - IU","m","15","15","30"]
["","Papildoma šaltnešio įkrova","","","kg/m","0,02 (ilgesniems kaip 10m vamzdžiams)","0,02 (ilgesniems kaip 10m vamzdžiams)","0,02 (ilgesniems kaip 10m vamzdžiams)"]
["","Lygio skirtumas","IU - OU","Maks.","m","12","12","20"]
["Standartiniai priedai","Installation manual","","","","1","1","1"]
["","Refrigerant charge label","","","","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1"]
["","General safety precautions","","","","1","1"]
["","Drain plug","","","","1","1","1"]
["El. tiekimas","Fazė","","","","1~","1~","1~"]
["Maitinimas","Dažnis","","","Hz","50","50","50"]
["","Įtampa","","","V","220-240","220-240","220-240"]
["Kompresorius","Tipas","","","","Hermetiškai užsandarintas stūmoklinis kompresorius","","Hermetiškai užsandarintas stūmoklinis kompresorius"]
["Standartiniai priedai","Drain cap","","","","","","3"]