{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":10,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXL-K"]
[]
[]
[]
[]
["","","","","","RXL20K3V1B","RXL25K3V1B","RXL35K2V1B","RXL42K2V1B","RXL50K2V1B"]
["Ventiliatorius","Oro debitas","Vėsinimas","Labai lėtai","m³/min.","","","30.1","30.6","48.9"]
["","","Šildymas","Labai lėtai","m³/min.","","","25.6","27.2","43.1"]
["","","","Labai lėtai","cfm","","","1063","1080","1727"]
["","","Šildymas","Labai lėtai","cfm","","","904","960","1522"]
["Matmenys","Įrenginys","","Aukštis","mm","550","550","550","550","735"]
["","","","Plotis","mm","765","765","765","765","825"]
["","","","Gylis","mm","285","285","285","285","300"]
["Svoris","Įrenginys","","","kg","34","34","34","39","47"]
["Ventiliatoriaus variklis","Greitis","Vėsinimas","Labai lėtai","aps. / min.","780","780","780","790","670"]
["","","Šildymas","Labai lėtai","aps. / min.","740","740","740","780","670"]
["Kompresorius","Type","","","","Hermetiškai užsandarintas stūmoklinis kompresorius","Hermetiškai užsandarintas stūmoklinis kompresorius","Hermetiškai užsandarintas stūmoklinis kompresorius","Hermetiškai užsandarintas stūmoklinis kompresorius","Hermetiškai užsandarintas stūmoklinis kompresorius"]
["Veikimo diapazonas","Aušinimas","Aplinkos","Min.","°C DB","-10","-10","-10","-10","-10"]
["","","","Maks.","°C DB","46","46","46","46","46"]
["","Šildymas","Aplinkos","Min.","°CWB","-25","-25","-25","-25","-25"]
["","","","Maks.","°CWB","18","18","18","18","18"]
["Garso slėgio lygis","Aušinimas","","Aukštas","dBA","46","46","48","48","48"]
["","Šildymas","","Aukštas","dBA","47","47","48","48","48"]
["Šaltnešis","Tipas","","","","R-410A","R-410A","R-410A","R-410A","R-410A"]
["Aušinimo medžiaga","Užpildytas kiekis","","","kg","1.0","1.05","1.2","1.3","1.7"]
["Šaltnešis","Užpildas","","","tCO2Eq","2.1","2.2","2.5","2.7","3.5"]
["Aušinimo medžiaga","GWP","","","","2087.5","2087.5","2087.5","2087.5","2087.5"]
["Vamzdžių jungtys","Vamzdžių ilgis","Maks.","OU - IU","m","20","20","20","20","30"]
["","Papildoma šaltnešio įkrova","","","kg/m","0,02 (ilgesniems kaip 10m vamzdžiams)","0,02 (ilgesniems kaip 10m vamzdžiams)","0,02 (ilgesniems kaip 10m vamzdžiams)","0,02 (ilgesniems kaip 10m vamzdžiams)","0,02 (ilgesniems kaip 10m vamzdžiams)"]
["","Lygio skirtumas","IU - OU","Maks.","m","15","15","15","15","20"]
["Standartiniai priedai","Installation manual","","","","1","1","1","1","1"]
["","Drain plug","","","","1"]
["El. tiekimas","Fazė","","","","1~","1~","1~","1~","1~"]
["Maitinimas","Dažnis","","","Hz","50","50","50","50","50"]
["","Įtampa","","","V","220-240","220-240","220-230-240","220-230-240","220-230-240"]
["Pastabos","","","","","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V"]
["","","","","","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V"]
["","","","","","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V"]