{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":11,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXP-N9"]
[]
[]
[]
[]
["","","","","","RXP20N5V1B9","RXP25N5V1B9","RXP35N5V1B9","RXP50N5V1B9","RXP60N5V1B9","RXP71N5V1B9"]
["Matmenys","Įrenginys","","Aukštis","mm","556","556","556","734","734","734"]
["","","","Plotis","mm","740","740","740","954","954","954"]
["","","","Gylis","mm","343","343","343","401","401","401"]
["Svoris","Įrenginys","","","kg","24","24","26","46","50","50"]
["Kompresorius","Tipas","","","","Hermetiškai užsandarintas stūmoklinis kompresorius","Hermetiškai užsandarintas stūmoklinis kompresorius","Hermetiškai užsandarintas stūmoklinis kompresorius"]
["Veikimo diapazonas","Aušinimas","Aplinkos","Min.","°CDB","-10","-10","-10"]
["","","","Maks.","°CDB","48","48","48"]
["","Šildymas","Aplinkos","Min.","° CWB","-15","-15","-15"]
["","","","Maks.","° CWB","18","18","18"]
["Garso slėgio lygis","Aušinimas","","Aukštas","dBA","46","46","48"]
["","","","Nom.","dBA","","","","47","49","52"]
["","Šildymas","","Aukštas","dBA","47","47","48"]
["","","","Nom.","dBA","","","","49","49","52"]
["Šaltnešis","Tipas","","","","R-32","R-32","R-32","R-32","R-32","R-32"]
["Aušinimo medžiaga","Užpildytas kiekis","","","kg","0.55","0.55","0.70","0.9","1.15","1.15"]
["Šaltnešis","Užpildas","","","tCO2Eq","0.37","0.37","0.48","0.61","0.78","0.78"]
["Aušinimo medžiaga","GWP","","","","675.0","675.0","675.0","675","675","675"]
["Vamzdžių jungtys","Vamzdžių ilgis","Maks.","OU - IU","m","20","20","20","30","30","30"]
["","Papildoma šaltnešio įkrova","","","kg/m","0,02 (ilgesniems kaip 10m vamzdžiams)","0,02 (ilgesniems kaip 10m vamzdžiams)","0,02 (ilgesniems kaip 10m vamzdžiams)","0,02 (ilgesniems kaip 10m vamzdžiams)","0,02 (ilgesniems kaip 10m vamzdžiams)","0,02 (ilgesniems kaip 10m vamzdžiams)"]
["","Lygio skirtumas","IU - OU","Maks.","m","12","12","12","20","20","20"]
["Standartiniai priedai","Installation manual","","","","1","1","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1","1","1"]
["","General safety precautions","","","","1","1","1"]
["","Drain plug","","","","1","1","1","1","1","1"]
["El. tiekimas","Fazė","","","","1~","1~","1~","1~","1~","1~"]
["Maitinimas","Dažnis","","","Hz","50","50","50","50","50","50"]
["","Įtampa","","","V","220-240","220-240","220-240","220-240","220-240","220-240"]
["Kompresorius","Tipas","","","","","","","Hermetiškai užsandarintas stūmoklinis kompresorius","Hermetiškai užsandarintas stūmoklinis kompresorius","Hermetiškai užsandarintas stūmoklinis kompresorius"]
["Standartiniai priedai","Drain cap","","","","","","","3","3","3"]
["Energijos naudojimo efektyvumo klasė","","","","","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Pastabos","","","","","","","","(1) - Žr. specialų darbinio diapazono brėžinį","(1) - Žr. specialų darbinio diapazono brėžinį","(1) - Žr. specialų darbinio diapazono brėžinį"]
["","","","","","","","","(2) - Žr. atskirą elektros duomenų brėžinį","(2) - Žr. atskirą elektros duomenų brėžinį","(2) - Žr. atskirą elektros duomenų brėžinį"]
["","","","","","","","","(3) - Yra floruotų šiltnamio efektą skatinančių dujų","(3) - Yra floruotų šiltnamio efektą skatinančių dujų","(3) - Yra floruotų šiltnamio efektą skatinančių dujų"]