{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":56,"n_cols":11,"rows_kept":56,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-F"]
[]
[]
[]
[]
["","","","","","RXS60F4V1B","RXS60F2V1B","RXS60F3V1B","RXS71FAV1B9","RXS71FV1B","RXS71FAV1B"]
["Garso slėgio lygis","Šildymas","","Aukštas","dBA","49","","","52"]
["","","","Žemas","dBA","46","","","49"]
["","Aušinimas","","Žemas","dBA","46","","","49"]
["","","","Aukštas","dBA","49","","","52"]
["Standartiniai priedai","Drenavimo mova","","","","1","","","1"]
["","Įrengimo vadovas","","","","1","","","1"]
["Šaltnešis","Charge","","","TCO2Eq","3.1","","","4.8"]
["","GWP","","","","2,087.5","","","2,087.5"]
["","Charge","","","kg","1.5","","","2.3"]
["","Tipas","","","","R-410A","","","R-410A"]
["Vamzdžių jungtys","Lygio skirtumas","IU - OU","Maks.","m","20","","","20"]
["","Papildoma šaltnešio įkrova","","","kg/m","0,02 (ilgesniems kaip 10m vamzdžiams)","","","0,02 (ilgesniems kaip 10m vamzdžiams)"]
["Compressor","Type","","","","Hermetiškai užsandarintas stūmoklinis kompresorius","","","Hermetiškai užsandarintas stūmoklinis kompresorius"]
["Matmenys","Įrenginys","","Plotis","mm","825","","","900"]
["","","","Depth","mm","300","","","320"]
["","","","Aukštis","mm","735","","","770"]
["Svoris","Įrenginys","","","kg","48","","","71"]
["Power supply","Fazė","","","","1~","","","1~"]
["","Dažnis","","","Hz","50","","","50"]
["","Įtampa","","","V","220-240","","","220-240"]
["Pastabos","","","","","(1) - SL: tyli ventiliatoriaus oro srauto dažnio nustatymuose","(1) - 220 V","","(1) - SL: tyli ventiliatoriaus oro srauto dažnio nustatymuose","(1) - 220 V"]
["","","","","","(2) - Yra floruotų šiltnamio efektą skatinančių dujų","(2) - 230 V","","(2) - Yra floruotų šiltnamio efektą skatinančių dujų","(2) - 230 V"]
["Matmenys","Įrenginys","","Aukštis","mm","","735","735","","770","770"]
["","","","Plotis","mm","","825","825","","900","900"]
["","","","Gylis","mm","","300","300","","320","320"]
["Svoris","Įrenginys","","","kg","","48","48","","71","71"]
["Compressor","Type","","","","","Hermetiškai užsandarintas stūmoklinis kompresorius","Hermetiškai užsandarintas stūmoklinis kompresorius","","Hermetiškai užsandarintas stūmoklinis kompresorius","Hermetiškai užsandarintas stūmoklinis kompresorius"]
["Veikimo diapazonas","Aušinimas","Aplinkos","Min.","°CDB","","-10","-10","","-10","-10"]
["","","","Maks.","°CDB","","46","46","","46","46"]
["","Šildymas","Aplinkos","Min.","°CWB","","-15","-15","","-15","-15"]
["","","","Maks.","°CWB","","18","20","","18","20"]
["Garso slėgio lygis","Aušinimas","","Aukštas","dBA","","49","49","","52","52"]
["","","","Žemas","dBA","","46","46","","49","49"]
["","Šildymas","","Aukštas","dBA","","49","49","","52","52"]
["","","","Žemas","dBA","","46","46","","49","49"]
["Šaltnešis","Tipas","","","","","R-410A","R-410A","","R-410A","R-410A"]
["Aušinimo medžiaga","Užpildytas kiekis","","","kg","","1.5","1.5","","2.3","2.3"]
["Šaltnešis","Užpildas","","","tCO2Eq","","3.1","3.1","","4.8","4.8"]
["Aušinimo medžiaga","GWP","","","","","2087.5","2087.5","","2087.5","2087.5"]
["Vamzdžių jungtys","Vamzdžių ilgis","Maks.","OU - IU","m","","30","30","","30","30"]
["","Papildoma šaltnešio įkrova","","","kg/m","","0,02 (ilgesniems kaip 10m vamzdžiams)","0,02 (ilgesniems kaip 10m vamzdžiams)","","0,02 (ilgesniems kaip 10m vamzdžiams)","0,02 (ilgesniems kaip 10m vamzdžiams)"]
["","Lygio skirtumas","IU - OU","Maks.","m","","20","20","","20","20"]
["Standartiniai priedai","Installation manual","","","","","Installation manual","1","","Installation manual","1"]
["","Drain plug","","","","","Drain plug","","","Drain plug"]
["El. tiekimas","Fazė","","","","","1~","1~","","1~","1~"]
["Maitinimas","Dažnis","","","Hz","","50","50","","50","50"]
["","Įtampa","","","V","","220-240","220-240","","220-240","220-240"]
["Pastabos","","","","","","(3) - 240 V","","","(3) - 240 V"]
["Standartiniai priedai","Drain socket","","","","","","1","","","1"]
["Triukšmingumo lygis","Vėsinimas","","","dBA","","","","65"]