{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":6,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-F8"]
[]
[]
[]
[]
["","","","","","RXS71FAV1B8"]
["Ventiliatorius","Oro debitas","Vėsinimas","Labai lėtai","m³/min.","46.0"]
["","","Šildymas","Labai lėtai","m³/min.","46.0"]
["","","","Labai lėtai","cfm","1624"]
["","","Šildymas","Labai lėtai","cfm","1624"]
["Matmenys","Įrenginys","","Aukštis","mm","770"]
["","","","Plotis","mm","900"]
["","","","Gylis","mm","320"]
["Svoris","Įrenginys","","","kg","71"]
["Ventiliatoriaus variklis","Greitis","Vėsinimas","Labai lėtai","rpm","730"]
["","","Šildymas","Labai lėtai","rpm","730"]
["Kompresorius","Tipas","","","","Hermetiškai užsandarintas stūmoklinis kompresorius"]
["Veikimo diapazonas","Aušinimas","Aplinkos","Min.","°C DB","-10"]
["","","","Maks.","°C DB","46"]
["","Šildymas","Aplinkos","Min.","° CWB","-15"]
["","","","Maks.","° CWB","18"]
["Garso slėgio lygis","Aušinimas","","Aukštas","dBA","52"]
["","Šildymas","","Aukštas","dBA","52"]
["Šaltnešis","Tipas","","","","R-410A"]
["Aušinimo medžiaga","Užpildytas kiekis","","","kg","2.3"]
["Šaltnešis","Užpildas","","","tCO2Eq","4.8"]
["Aušinimo medžiaga","GWP","","","","2087.5"]
["Vamzdžių jungtys","Vamzdžių ilgis","Maks.","OU - IU","m","30"]
["","Papildoma šaltnešio įkrova","","","kg/m","0,02 (ilgesniems kaip 10m vamzdžiams)"]
["","Lygio skirtumas","IU - OU","Maks.","m","20"]
["Standartiniai priedai","Installation manual","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","Drain socket assy","","","","1"]
["El. tiekimas","Fazė","","","","1~"]
["Maitinimas","Dažnis","","","Hz","50"]
["","Įtampa","","","V","220-240"]
["Pastabos","","","","","(1) - 220 V"]
["","","","","","(2) - 230 V"]
["","","","","","(3) - 240 V"]