{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":72,"n_cols":8,"rows_kept":72,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-L3"]
[]
[]
[]
[]
["","","","","","RXS20L3V1B","RXS25L3V1B","RXS35L3V1B"]
["Garso slėgio lygis","Šildymas","","Aukštas","dBA","","","48"]
["","Aušinimas","","Aukštas","dBA","","","48"]
["Standartiniai priedai","Įrengimo vadovas","","","","","","1"]
["","Užpildymo šaltnešiu etiketė","","","","","","1"]
["","Etiketės apie floruotas šiltnamio efektą skatinančias dujas įvairiomis kalbomis","","","","","","1"]
["","Išleidimo kaištis (tik šildymo siurblio modeliams)","","","","","","1"]
["Aušinimo medžiaga","Charge","","","TCO2Eq","","","2.5"]
["","GWP","","","","","","2,087.5"]
["","Charge","","","kg","","","1.2"]
["","Tipas","","","","","","R-410A"]
["Ventiliatoriaus variklis","Greitis","Aušinimas","Labai lėtai","rpm","","","780"]
["","","Šildymas","Labai lėtai","rpm","","","740"]
["Veikimo diapazonas","Aušinimas","Aplinkos","Maks.","°CDB","","","46"]
["","","","Min.","°CDB","","","-10"]
["","Šildymas","Aplinkos","Maks.","° CWB","","","18"]
["","","","Min.","° CWB","","","-15"]
["Vamzdžių jungtys","Lygių skirtumas","IU - OU","Maks.","m","","","15"]
["","Papildoma šaltnešio įkrova","","","kg/m","","","0,02 (ilgesniems kaip 10m vamzdžiams)"]
["Kompresorius","Tipas","","","","","","Hermetiškai užsandarintas stūmoklinis kompresorius"]
["Matmenys","Įrenginys","","Plotis","mm","","","765"]
["","","","Gylis","mm","","","285"]
["","","","Aukštis","mm","","","550"]
["Svoris","Įrenginys","","","kg","","","34"]
["Ventiliatorius","Oro debitas","Šildymas","Labai lėtai","cfm","","","904"]
["","","","Labai lėtai","m³/min.","","","25.6"]
["","","Aušinimas","Labai lėtai","m³/min.","","","30.1"]
["","","","Labai lėtai","cfm","","","1,063"]
["Power supply","Fazė","","","","","","1~"]
["","Dažnis","","","Hz","","","50"]
["","Įtampa","","","V","","","220-240"]
["Pastabos","","","","","","","(1) - SL: tyli ventiliatoriaus oro srauto dažnio nustatymuose"]
["Ventiliatorius","Oro debitas","Vėsinimas","Labai lėtai","m³/min.","30.1","30.1"]
["","","Šildymas","Labai lėtai","m³/min.","25.6","25.6"]
["","","","Labai lėtai","cfm","1063","1063"]
["","","Šildymas","Labai lėtai","cfm","904","904"]
["Matmenys","Įrenginys","","Aukštis","mm","550","550"]
["","","","Plotis","mm","765","765"]
["","","","Gylis","mm","285","285"]
["Svoris","Įrenginys","","","kg","34","34"]
["Ventiliatoriaus variklis","Greitis","Vėsinimas","Labai lėtai","rpm","780","780"]
["","","Šildymas","Labai lėtai","rpm","740","740"]
["Kompresorius","Tipas","","","","Hermetiškai užsandarintas stūmoklinis kompresorius","Hermetiškai užsandarintas stūmoklinis kompresorius"]
["Veikimo diapazonas","Aušinimas","Aplinkos","Min.","°CDB","-10","-10"]
["","","","Maks.","°CDB","46","46"]
["","Šildymas","Aplinkos","Min.","° CWB","-15","-15"]
["","","","Maks.","° CWB","18","18"]
["Garso slėgio lygis","Aušinimas","","Aukštas","dBA","46","46"]
["","Šildymas","","Aukštas","dBA","47","47"]
["Šaltnešis","Tipas","","","","R-410A","R-410A"]
["Aušinimo medžiaga","Užpildytas kiekis","","","kg","1.0","1.0"]
["Šaltnešis","Užpildas","","","tCO2Eq","2.1","2.1"]
["Aušinimo medžiaga","GWP","","","","2087.5","2087.5"]
["Vamzdžių jungtys","Vamzdžių ilgis","Maks.","OU - IU","m","20","20"]
["","Papildoma šaltnešio įkrova","","","kg/m","0,02 (ilgesniems kaip 10m vamzdžiams)","0,02 (ilgesniems kaip 10m vamzdžiams)"]
["","Lygio skirtumas","IU - OU","Maks.","m","15","15"]
["Standartiniai priedai","Installation manual","","","","1","1"]
["","Refrigerant charge label","","","","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1"]
["","Drain plug","","","","1"]
["El. tiekimas","Fazė","","","","1~","1~"]
["Maitinimas","Dažnis","","","Hz","50","50"]
["","Įtampa","","","V","220-240","220-240"]
["Pastabos","","","","","(1) - 220 V"]
["","","","","","(2) - 230 V"]
["","","","","","(3) - 240 V"]
["Standartiniai priedai","Drain plug (only heat pump models)","","","","","1"]