{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":7,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZA-D"]
[]
[]
[]
[]
["","","","","","RZA200D7Y1B","RZA250D7Y1B"]
["Matmenys","Vienetas","","Aukštis","mm","870","870"]
["","","","Plotis","mm","1,100","1,100"]
["","","","Gylis","mm","460","460"]
["Svoris","Vienetas","","","kg","117","117"]
["Kompresorius","Tipas","","","","Hermetiškai užsandarintas spiralinis kompresorius","Hermetiškai užsandarintas spiralinis kompresorius"]
["Veikimo diapazonas","Vėsinimas","Aplinkos","Min.","°CDB","-20","-20"]
["","","","Maks.","°CDB","46","46"]
["","Šildymas","Aplinkos","Min.","° CWB","-20","-20"]
["","","","Maks.","° CWB","15","15"]
["Garso galingumo lygis","Vėsinimas","","","dBA","73","76"]
["","Šildymas","","","dBA","76 (1)","79 (1)"]
["Garso slėgio lygis","Aušinimas","","Nom.","dBA","53","57"]
["","Šildymas","","Nom.","dBA","60","63"]
["Šaltnešis","Type","","","","R-32","R-32"]
["","Įkrova","","","kg","5","5"]
["","GWP","","","","675","675"]
["Vamzdžių jungtys","Skysčių vamzdis","","OD","mm","9.52","9.52"]
["","Dujos","","Iš. diam.","mm","22.2","22.2"]
["","Vamzdžių ilgis","Maks.","OU - IU","m","100","100"]
["","","Sistema","Neutralus","m","30","30"]
["","Papildoma šaltnešio įkrova","","","kg/m","Žr. įrengimo vadovą","Žr. įrengimo vadovą"]
["Standartiniai priedai","Įrengimo vadovas","","","","1","1"]
["","Bendrosios saugos priemonės","","","","1","1"]
["","Sujungimų apvyniojimai","","","","2","2"]
["","Nulupama F tipo dujų etiketė","","","","1","1"]
["","Sujungimo vamzdžiai","","","","6","6"]
["Power supply","Fazė","","","","3~","3~"]
["","Dažnis","","","Hz","50","50"]
["","Įtampa","","","V","380-415","380-415"]
["Srovė – 50Hz","Maksimali saugiklių srovė (MFA)","","","A","20","20"]
["Pastabos","","","","","(1) - Pagal ENER part. 21","(1) - Pagal ENER part. 21"]