{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":8,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZAG-B"]
[]
[]
[]
[]
["","","","","","RZAG35B5V1B","RZAG50B5V1B","RZAG60B5V1B"]
["Matmenys","Įrenginys","","Aukštis","mm","734","734","734"]
["","","","Plotis","mm","870","870","870"]
["","","","Gylis","mm","373","373","373"]
["Svoris","Įrenginys","","","kg","52","52","52"]
["Kompresorius","Tipas","","","","Hermetiškai užsandarintas stūmoklinis kompresorius","Hermetiškai užsandarintas stūmoklinis kompresorius","Hermetiškai užsandarintas stūmoklinis kompresorius"]
["Veikimo diapazonas","Aušinimas","Aplinkos","Min.","°C DB","-20","-20","-20"]
["","","","Maks.","°C DB","52","52","52"]
["","Šildymas","Aplinkos","Min.","° CWB","-21","-21","-21"]
["","","","Maks.","° CWB","18","18","18"]
["Garso galingumo lygis","Vėsinimas","","","dBA","62","63","64"]
["","Šildymas","","","dBA","62","63","64"]
["Garso slėgio lygis","Aušinimas","","Nom.","dBA","48","49","50"]
["","Šildymas","","Nom.","dBA","48","49","50"]
["Šaltnešis","Tipas","","","","R-32","R-32","R-32"]
["Aušinimo medžiaga","Užpildytas kiekis","","","kg","1.55","1.55","1.55"]
["","GWP","","","","675","675","675"]
["Šaltnešis","Užpildas","","","tCO2Eq","1.05","1.05","1.05"]
["Vamzdžių jungtys","Skystis","","OD","mm","6.35","6.35","6.35"]
["","Dujos","","Iš. diam.","mm","9.52","12.7","12.7"]
["","Vamzdžių ilgis","Maks.","OU - IU","m","50","50","50"]
["","Papildoma šaltnešio įkrova","","","kg/m","0,02 (ilgesniems kaip 30m vamzdžiams)","0,02 (ilgesniems kaip 30m vamzdžiams)","0,02 (ilgesniems kaip 30m vamzdžiams)"]
["","Lygio skirtumas","IU - OU","Maks.","m","30","30","30"]
["Standartiniai priedai","RZAG35B5V1B","","","","1"]
["","Installation manual","","","","1","1","1"]
["","Refrigerant charge label","","","","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1"]
["","General safety precautions","","","","General safety precautions","General safety precautions","General safety precautions"]
["","LOT10 Energy Label","","","","LOT10 Energy Label","LOT10 Energy Label","LOT10 Energy Label"]
["","Drain cap","","","","3","3","3"]
["","Drain plug","","","","1","1","1"]
["El. tiekimas","Fazė","","","","1~","1~","1~"]
["Maitinimas","Dažnis","","","Hz","50","50","50"]
["","Įtampa","","","V","220-240","220-240","220-240"]
["Pastabos","","","","","(1) - Žr. specialų darbinio diapazono brėžinį","(1) - Žr. specialų darbinio diapazono brėžinį","(1) - Žr. specialų darbinio diapazono brėžinį"]
["","","","","","(2) - Žr. atskirą elektros duomenų brėžinį","(2) - Žr. atskirą elektros duomenų brėžinį","(2) - Žr. atskirą elektros duomenų brėžinį"]
["","","","","","(3) - Yra floruotų šiltnamio efektą skatinančių dujų","(3) - Yra floruotų šiltnamio efektą skatinančių dujų","(3) - Yra floruotų šiltnamio efektą skatinančių dujų"]
["Standartiniai priedai","RZAG50B5V1B","","","","","1"]
["","RZAG60B5V1B","","","","","","1"]