{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":74,"n_cols":9,"rows_kept":74,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZAG-MV1"]
[]
[]
[]
[]
["","","","","","RZAG71M7V1B","RZAG100M7V1B","RZAG125M7V1B","RZAG140M7V1B"]
["Garso slėgio lygis","Šildymas","","Nom.","dBA","","","","52"]
["","Aušinimas","","Nom.","dBA","","","","51"]
["Standartiniai priedai","Sujungimų apvyniojimai","","","","","","","2"]
["","Įrengimo vadovas","","","","","","","1"]
["","F tipo dujų kontrolės šaltnešio etiketė","","","","","","","1"]
["","Bendrosios saugos priemonės","","","","","","","1"]
["","LOT10 energijos suvartojimo etiketė","","","","","","","1"]
["Aušinimo medžiaga","Charge","","","TCO2Eq","","","","2.53"]
["","GWP","","","","","","","675"]
["","Charge","","","kg","","","","3.75"]
["","Tipas","","","","","","","R-32"]
["Vamzdžių jungtys","Skystis","","OD","mm","","","","9.52"]
["","Vamzdžių ilgis","Maks.","OU - IU","m","","","","85"]
["","","Sistema","Neutralus","m","","","","40"]
["","","","Ekvivalentas","m","","","","100"]
["","Dujos","","Iš. diam.","mm","","","","15.9"]
["","Lygių skirtumas","IU - IU","Maks.","m","","","","0.5"]
["","","IU - OU","Maks.","m","","","","30.0"]
["","Papildoma šaltnešio įkrova","","","kg/m","","","","Žr. įrengimo vadovą"]
["Sound power level","Vėsinimas","","","dBA","","","","70"]
["","Šildymas","","","dBA","","","","70 (1)"]
["Kompresorius","Tipas","","","","","","","Hermetiškai užsandarintas stūmoklinis kompresorius"]
["Matmenys","Įrenginys","","Plotis","mm","","","","940"]
["","","","Gylis","mm","","","","320"]
["","","","Aukštis","mm","","","","1,430"]
["Svoris","Įrenginys","","","kg","","","","92"]
["Power supply","Fazė","","","","","","","1~"]
["","Dažnis","","","Hz","","","","50"]
["","Įtampa","","","V","","","","220-240"]
["Pastabos","","","","","","","","(1) - Pagal ENER part. 21"]
["","","","","","","","","(2) - Europos/tarptautinis techninis standartas, nustatantis ribines prie bendrųjų žemosios įtampos tinklų, kurių vienos fazės maitinimo srovė didesnė kaip 16 A ir <= 75 A, prijungto įrenginio gaminamų harmoninių srovių vertes"]
["","","","","","","","","(3) - Ssc: trumpojo jungimo galia"]
["","","","","","","","","(4) - Europos / tarptautinis techninis standartas, nustatantis ribines prie bendrųjų žemosios įtampos tinklų, kurių vienos fazės maitinimo srovė ≤ 16 A, prijungtos įrangos gaminamų harmoninių srovių vertes."]
["Matmenys","Įrenginys","","Aukštis","mm","990","1430","1430"]
["","","","Plotis","mm","940","940","940"]
["","","","Gylis","mm","320","320","320"]
["Svoris","Įrenginys","","","kg","70","92","92"]
["Kompresorius","Tipas","","","","Hermetiškai užsandarintas stūmoklinis kompresorius","Hermetiškai užsandarintas stūmoklinis kompresorius","Hermetiškai užsandarintas stūmoklinis kompresorius"]
["Veikimo diapazonas","Aušinimas","Aplinkos","Min.","°CDB","-20","-20","-20"]
["","","","Maks.","°CDB","52","52","52"]
["","Šildymas","Aplinkos","Min.","° CWB","-20","-20","-20"]
["","","","Maks.","° CWB","18.0","18.0","18.0"]
["Garso galingumo lygis","Vėsinimas","","","dBA","64","66","69"]
["Garso slėgio lygis","Aušinimas","","Nom.","dBA","46","47","50"]
["","Šildymas","","Nom.","dBA","49","51","52"]
["Šaltnešis","Tipas","","","","R-32","R-32","R-32"]
["Aušinimo medžiaga","Užpildytas kiekis","","","kg","2.95","3.75","3.75"]
["","GWP","","","","675","675","675"]
["Šaltnešis","Užpildas","","","tCO2Eq","1.99","2.53","2.53"]
["Vamzdžių jungtys","Skystis","","OD","mm","9.52","9.52","9.52"]
["","Dujos","","Iš. diam.","mm","15.9","15.9","15.9"]
["","Vamzdžių ilgis","Maks.","OU - IU","m","55","85","85"]
["","","Sistema","Ekvivalentas","m","75","100","100"]
["","","","Neutralus","m","40","40","40"]
["","Papildoma šaltnešio įkrova","","","kg/m","Žr. įrengimo vadovą","Žr. įrengimo vadovą","Žr. įrengimo vadovą"]
["","Lygio skirtumas","IU - OU","Maks.","m","30.0","30.0","30.0"]
["","","IU - IU","Maks.","m","0.5","0.5","0.5"]
["Standartiniai priedai","Installation manual","","","","1","1","1"]
["","Refrigerant label for F-gas regulation","","","","1","1","1"]
["","General safety precautions","","","","1","1","1"]
["","LOT10 Energy Label","","","","1","1","1"]
["","Tie-wraps","","","","2","2","2"]
["El. tiekimas","Fazė","","","","1~","1~","1~"]
["Maitinimas","Dažnis","","","Hz","50","50","50"]
["","Įtampa","","","V","220-240","220-240","220-240"]
["Srovė – 50 Hz","Maksimali saugiklių srovė (MFA)","","","A","20","32","32"]
["Garso galingumo lygis","Šildymas","","","dBA","","","69 (1)"]
["Pastabos","","","","","","","(1) - Pagal ENER part. 21"]