{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":13,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZAG-NV1"]
[]
[]
[]
[]
["","","","","","RZAG71N7V1B","RZAG71N2V1B","RZAG100N7V1B","RZAG100N2V1B","RZAG125N7V1B","RZAG125N2V1B","RZAG140N7V1B","RZAG140N2V1B"]
["Matmenys","Įrenginys","","Aukštis","mm","870","870","870","870","870","870","870","870"]
["","","","Plotis","mm","1100","1100","1100","1100","1100","1100","1100","1100"]
["","","","Gylis","mm","460","460","460","460","460","460","460","460"]
["Svoris","Įrenginys","","","kg","81","81","85","85","95","95","95","95"]
["Kompresorius","Type","","","","","","Hermetiškai užsandarintas stūmoklinis kompresorius","Hermetiškai užsandarintas stūmoklinis kompresorius","Hermetiškai užsandarintas stūmoklinis kompresorius","Hermetiškai užsandarintas stūmoklinis kompresorius","Hermetiškai užsandarintas stūmoklinis kompresorius","Hermetiškai užsandarintas stūmoklinis kompresorius"]
["Veikimo diapazonas","Aušinimas","Aplinkos","Min.","°C DB","-20","-20","-20","-20","-20","-20","-20","-20"]
["","","","Maks.","°C DB","52","52","52","52","52","52","52","52"]
["","Šildymas","Aplinkos","Min.","°CWB","-20","-20","-20","-20","-20","-20","-20","-20"]
["","","","Maks.","°CWB","18","18","18","18","18","18","18","18"]
["Garso galingumo lygis","Vėsinimas","","","dBA","64","64","66","66","69","69","70","70"]
["","Šildymas","","","dBA","","","","","68 (1)","68 (1)","71 (1)","71 (1)"]
["Garso slėgio lygis","Aušinimas","","Nom.","dBA","46","46","47","47","49","49","50","50"]
["","Šildymas","","Nom.","dBA","48","48","50","50","52","52","52","52"]
["Šaltnešis","Tipas","","","","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32"]
["Aušinimo medžiaga","Užpildytas kiekis","","","kg","3.2","3.20","3.2","3.20","3.7","3.70","3.7","3.70"]
["","GWP","","","","675","675","675","675","675","675","675","675"]
["Šaltnešis","Užpildas","","","tCO2Eq","2.16","2.16","2.16","2.16","2.5","2.50","2.5","2.50"]
["Vamzdžių jungtys","Skystis","","OD","mm","10","10","10","10","10","10","10","10"]
["","Dujos","","Iš. diam.","mm","15.9","15.9","15.9","15.9","15.9","15.9","15.9","15.9"]
["","Vamzdžių ilgis","Maks.","OU - IU","m","55","55","85","85","85","85","85","85"]
["","","Sistema","Ekvivalentas","m","75","75","100","100","100","100","100","100"]
["","","","Neutralus","m","40","40","40","40","40","40","40","40"]
["","Papildoma šaltnešio įkrova","","","kg/m","Žr. įrengimo vadovą","Žr. įrengimo vadovą","Žr. įrengimo vadovą","Žr. įrengimo vadovą","Žr. įrengimo vadovą","Žr. įrengimo vadovą","Žr. įrengimo vadovą","Žr. įrengimo vadovą"]
["","Lygio skirtumas","IU - OU","Maks.","m","30","30","30","30","30","30","30","30"]
["","","IU - IU","Maks.","m","0.5","0.5","0.5","0.5","0.5","0.5","0.5","0.5"]
["Standartiniai priedai","Installation manual","","","","1","1","1","1","1","1","1","1"]
["","Refrigerant label for F-gas regulation","","","","1","1","1","1","1","1","1","1"]
["","General safety precautions","","","","1","1","1","1","1","1","1","1"]
["","Peel off F-gas label","","","","1","1","1","1","1","1","1","1"]
["","Tie-wraps","","","","2","2","2","2","2","2","2","2"]
["El. tiekimas","Fazė","","","","1~","1~","1~","1~","1~","1~","1~","1~"]
["Maitinimas","Dažnis","","","Hz","50","50","50","50","50","50","50","50"]
["","Įtampa","","","V","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]
["Srovė – 50 Hz","Maksimali saugiklių srovė (MFA)","","","A","20","20","32","32","32","32","32","32"]
["Kompresorius","Tipas","","","","Hermetiškai užsandarintas stūmoklinis kompresorius","Hermetiškai užsandarintas stūmoklinis kompresorius"]
["Pastabos","","","","","","","","","(1) - Pagal ENER part. 21","(1) - Pagal ENER part. 21","(1) - Pagal ENER part. 21","(1) - Pagal ENER part. 21"]