{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":54,"n_cols":7,"rows_kept":54,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZQ-C"]
[]
[]
[]
[]
["","","","","","RZQ200C7Y1B","RZQ250C7Y1B"]
["Matmenys","Vienetas","","Aukštis","mm","1,680"]
["","","","Plotis","mm","930"]
["","","","Gylis","mm","765"]
["Svoris","Įrenginys","","","kg","183.0"]
["Kompresorius","Tipas","","","","Hermetiškai užsandarintas spiralinis kompresorius"]
["Veikimo diapazonas","Aušinimas","Aplinkos","Min.","°CDB","-5.0"]
["","","","Maks.","°CDB","46.0"]
["","Šildymas","Aplinkos","Min.","°CWB","-15.0"]
["","","","Maks.","°CWB","15.0"]
["Garso galingumo lygis","Cooling","","","dBA","78.0"]
["","Šildymas","","","dBA","78.0"]
["Šaltnešis","Tipas","","","","R-410A"]
["","Įkrova","","","kg","8.3"]
["","GWP","","","","2,087.5"]
["Vamzdžių jungtys","Skystis","","OD","mm","9.52"]
["","Dujų vamzdis","","OD","mm","22.2"]
["","Vamzdžių ilgis","Maks.","OU - IU","m","100"]
["","","Sistema","Neutralus","m","30"]
["Standartiniai priedai","Įrengimo vadovas","","","","1"]
["","Sujungimo vamzdžiai","","","","4"]
["Power supply","Fazė","","","","3N~"]
["","Dažnis","","","Hz","50"]
["","Įtampa","","","V","380-415"]
["Srovė – 50 Hz","Maksimali saugiklių srovė (MFA)","","","A","25"]
["Pastabos","","","","","(1) - FDQ vidinio įrenginio maitinimas yra atskiras"]
["","","","","","(2) - Žr. atskirus elektros duomenų brėžinius"]
["Matmenys","Įrenginys","","Aukštis","mm","","1680"]
["","","","Plotis","mm","","930"]
["","","","Gylis","mm","","765"]
["Svoris","Įrenginys","","","kg","","184.0"]
["Kompresorius","Tipas","","","","","Hermetiškas sraigtinis kompresorius"]
["Veikimo diapazonas","Aušinimas","Aplinkos","Min.","°CDB","","-5.0"]
["","","","Maks.","°CDB","","46.0"]
["","Šildymas","Aplinkos","Min.","°CWB","","-15.0"]
["","","","Maks.","°CWB","","15.0"]
["Garso galingumo lygis","Vėsinimas","","","dBA","","78.0"]
["","Šildymas","","","dBA","","78.0"]
["Aušinimo medžiaga","Užpildytas kiekis","","","kg","","9.3"]
["","GWP","","","","","2087.5"]
["Šaltnešis","Užpildas","","","tCO2Eq","","19.4"]
["Vamzdžių jungtys","Skystis","","OD","mm","","12.70"]
["","Dujos","","Iš. diam.","mm","","22.2"]
["","Vamzdžių ilgis","Maks.","OU - IU","m","","100"]
["","","Sistema","Neutralus","m","","30"]
["Standartiniai priedai","Installation manual","","","","","1"]
["","Connection pipes","","","","","4"]
["Maitinimas","Dažnis","","","Hz","","50"]
["Srovė – 50 Hz","Maksimali saugiklių srovė (MFA)","","","A","","25"]