{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":5,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","WLCO2"]
[]
[]
[]
[]
["","","","","WLCO2."]
["Maksimalus jungiamų vidinių įrenginių skaičius","","","","0"]
["Maksimalus jungiamų lauko įrenginių skaičius @","","","","0"]
["Korpusas","Spalva","","","Balta"]
["Korpusas| Mygtuko dangtis","","","","Ne"]
["Korpusas| Veikimo LED","Spalva","","","Žalia"]
["Matmenys","Įrenginys","Aukštis","mm","95"]
["","","Plotis","mm","95.0"]
["","","Gylis","mm","62.0"]
["","Supakuotas įrenginys","Aukštis","mm","565"]
["","","Plotis","mm","375"]
["","","Gylis","mm","280"]
["Svoris","Įrenginys","","kg","0.126"]
["Pakuotė","Medžiaga","","","Kartonas"]
["","Svoris","","kg","0.046"]
["Aplinkos temperatūra","Veikimas","Min.","°C","-10"]
["","","Maks.","°C","50"]
["","Saugojimas","Min.","°C","-20"]
["","","Maks.","°C","60"]
["Aplinkos temperatūra| Santykinis drėgnumas <-=-%","%","","","90"]
["Įrengimas","","","","Vidaus įranga"]