{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":47,"n_cols":9,"rows_kept":47,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A"]
[]
[]
[]
[]
["","","","","","FBA35A2VEB","FBA50A2VEB","FBA60A2VEB","FBA71A2VEB"]
["Garso slėgio lygis","Šildymas","","Aukštas","dBA","37.0","37.0","31.0","31.0"]
["","","","Vidutinis","dBA","34.0","34.0","28.0","28.0"]
["","","","Žemas","dBA","29.0","29.0","25.0","25.0"]
["","Aušinimas","","Vidutinis","dBA","32.0","32.0","28.0","28.0"]
["","","","Žemas","dBA","29.0","29.0","25.0","25.0"]
["","","","Aukštas","dBA","35.0","35.0","30.0","30.0"]
["Standartiniai priedai","Eksploatavimo vadovas","","","","1","1","1","1"]
["","Įrengimo vadovas","","","","1","1","1","1"]
["","Drenavimo žarna","","","","1","1","1","1"]
["","Metaliniai veržtuvas drenažo žarnai","","","","1","1","1","1"]
["","Poveržlė kablio laikytuvui","","","","8","8","8","8"]
["","Varžtai","","","","40","40","40","40"]
["","Izoliacija priedui","","","","2","2","2","2"]
["","Sandarinimo tarpikliai","","","","5","5","5","5"]
["","Veržtuvai","","","","4","4","4","4"]
["Valdymo sistemos","Wired remote control","","","","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7"]
["","Infrared remote control","","","","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66"]
["Piping connections","Skystis","","OD","mm","6.35","6.35","6.35","9.52"]
["","Dujos","","Iš. diam.","mm","9.52","12.70","12.70","15.90"]
["","Drain","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Garso galingumo lygis","Vėsinimas","","","dBA","60","60","56","56"]
["Matmenys","Vienetas","","Plotis","mm","700","700","1,000","1,000"]
["","","","Gylis","mm","800","800","800","800"]
["","","","Aukštis","mm","245","245","245","245"]
["Korpusas","Medžiaga","","","","Galvanizuoto plieno plokštė","Galvanizuoto plieno plokštė","Galvanizuoto plieno plokštė","Galvanizuoto plieno plokštė"]
["","Colour","","","","Nedažytas (galvanizuotas)","Nedažytas (galvanizuotas)","Nedažytas (galvanizuotas)","Nedažytas (galvanizuotas)"]
["Svoris","Įrenginys","","","kg","28.0","28.0","35.0","35.0"]
["Ventiliatorius","Išorinis statinis slėgis","","Aukštas","Pa","150","150","150","150"]
["","","","Nom.","Pa","30","30","30","30"]
["","Oro debitas","Šildymas","Didelis","m³/min.","15.0","15.0","18.0","18.0"]
["","","","Mažas","m³/min.","10.5","10.5","12.5","12.5"]
["","","","Vidutinis","m³/min.","12.5","12.5","15.0","15.0"]
["","","Vėsinimas","Mažas","m³/min.","10.5","10.5","12.5","12.5"]
["","","","Vidutinis","m³/min.","12.5","12.5","15.0","15.0"]
["","","","Didelis","m³/min.","15.0","15.0","18.0","18.0"]
["Drenavimo aukštis","mm","","","","625","625","625","625"]
["Power supply","Phase","","","","1~","1~","1~","1~"]
["","Dažnis","","","Hz","50/60","50/60","50/60","50/60"]
["","Įtampa","","","V","220-240/220","220-240/220","220-240/220","220-240/220"]
["Pastabos","","","","","(1) - Garso galios lygis yra absoliuti reikšmė nurodanti galią, kurią sukuria garso šaltinis.","(1) - Garso galios lygis yra absoliuti reikšmė nurodanti galią, kurią sukuria garso šaltinis.","(1) - Garso galios lygis yra absoliuti reikšmė nurodanti galią, kurią sukuria garso šaltinis.","(1) - Garso galios lygis yra absoliuti reikšmė nurodanti galią, kurią sukuria garso šaltinis."]
["","","","","","(2) - Žr. atskirą elektros duomenų brėžinį","(2) - Žr. atskirą elektros duomenų brėžinį","(2) - Žr. atskirą elektros duomenų brėžinį","(2) - Žr. atskirą elektros duomenų brėžinį"]