{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":22,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A(9) / RZAG-A"]
[]
[]
[]
[]
["","","","","FHA35AVEB98 / RZAG35A2V1B","FHA50AVEB98 / RZAG35A2V1B","FHA50AVEB98 / RZAG50A2V1B","FHA71AVEB98 / RZAG60A2V1B","FHA60AVEB98 / RZAG50A2V1B","FHA60AVEB98 / RZAG60A2V1B","FHA35AVEB9 / RZAG35A2V1B (Archived)","FHA50AVEB9 / RZAG35A2V1B (Archived)","FHA35AVEB99 / RZAG35A2V1B (Archived)","FHA50AVEB99 / RZAG35A2V1B (Archived)","FHA50AVEB9 / RZAG50A2V1B (Archived)","FHA50AVEB99 / RZAG50A2V1B (Archived)","FHA60AVEB9 / RZAG50A2V1B (Archived)","FHA60AVEB9 / RZAG60A2V1B (Archived)","FHA71AVEB9 / RZAG60A2V1B (Archived)","FHA60AVEB99 / RZAG60A2V1B (Archived)","FHA60AVEB99 / RZAG50A2V1B (Archived)","FHA71AVEB99 / RZAG60A2V1B (Archived)"]
["Aušinimo galingumas","Min.","","kW","1.70","1.70","1.70","1.90","1.70","1.90","1.7","1.7","1.70","1.70","1.7","1.70","1.7","1.9","1.9","1.90","1.70","1.90"]
["","Maks.","","kW","4.50","4.50","6.00","6.80","6.00","6.80","4.5","4.5","4.50","4.50","6.0","6.00","6.0","6.8","6.8","6.80","6.00","6.80"]
["","Nom.","","kW","3.50","3.50","5.00","6.00","5.00","6.00","3.5","3.5","3.50","3.50","5.0","5.00","5.0","6.0","6.00","6.00","5.00","6.00"]
["Patalpos vėsinimas","SEER","","","6.40","6.65","6.80","6.81","7.02","6.60","6.40","6.65","6.40","6.65","6.80","6.80","7.02","6.60","6.81","6.60","7.02","6.81"]
["","Metinės energijos sąnaudos","","kWh/a","191","184","257","308","249","318","191","184","191","184","257","257","249","318","308","318","249","308"]
["","Vėsinimas","Pdesign","kW","3.50","3.50","5.00","6.00","5.00","6.00","3.50","3.50","3.50","3.50","5.00","5.00","5.00","6.00","6.00","6.00","5.00","6.00"]
["","Energijos efektyvumo klasė","","","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++"]
["Patalpos šildymas (vidutinis klimatas)","Pajėgumas","Pdesign","kW","3.10","3.10","4.00","4.60","4.00","4.60","3.10","3.10","3.10","3.10","4.00","4.00","4.00","4.60","4.60","4.60","4.00","4.60"]
["","SCOP/A","","","4.10","4.18","4.30","4.35","4.44","4.20","4.10","4.18","4.10","4.18","4.30","4.30","4.44","4.20","4.35","4.20","4.44","4.35"]
["","Energijos efektyvumo klasė","","","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+"]
["","Metinės energijos sąnaudos","","kWh/a","1,058","1,038","1,302","1,480","1,261","1,633","1,058","1,038","1,058","1,038","1,302","1,302","1,261","1,633","1,480","1,633","1,261","1,480"]
["Vardinis našumas","Annual energy consumption","","kWh","380","347","610","690","590","769","380","347","380","347","610","610","590","769","690","769","590","690"]
["","EER","","","4.60","5.05","4.10","4.35","4.24","3.90","4.60","5.05","4.60","5.05","4.10","4.10","4.24","3.90","4.35","3.90","4.24","4.35"]
["","COP","","","4.10","4.18","3.71","3.52","3.75","3.40","4.10","4.18","4.10","4.18","3.71","3.71","3.75","3.40","3.52","3.40","3.75","3.52"]
["","Energijos suvartojimo ženklinimo direktyva","Vėsinimas","","A","A","A","A","A","A","A","A","A","A","A","A","A","A","A","A","A","A"]
["","","Šildymas","","A","A","A","B","A","C","A","A","A","A","A","A","A","C","B","C","A","B"]
["Šildymo galia","Nom.","","kW","4.00","4.00","5.80","7.00","6.00","7.00","4.00","4.00","4.00","4.00","5.80","5.80","6.00","7.00","7.00","7.00","6.00","7.00"]
["","Min.","","kW","1.40","1.40","1.70","1.70","1.70","1.70","1.40","1.40","1.40","1.40","1.70","1.70","1.70","1.70","1.70","1.70","1.70","1.70"]
["","Maks.","","kW","5.50","5.50","6.50","7.50","6.50","7.50","5.50","5.50","5.50","5.50","6.50","6.50","6.50","7.50","7.50","7.50","6.50","7.50"]