{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":13,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-R"]
[]
[]
[]
[]
["","","","","","FTXM20R2V1B","FTXM20R5V1B","FTXM35R5V1B","FTXM35R2V1B","FTXM42R5V1B","FTXM42R2V1B","FTXM50R2V1B","FTXM60R2V1B"]
["Tiekiama galia","Aušinimas","","Nom.","kW","0.029","0.029","0.03","0.03","0.034","0.034","0.03","0.032"]
["","Šildymas","","Nom.","kW","0.023","0.023","0.027","0.027","0.038","0.038","0.032","0.035"]
["Korpusas","Spalva","","","","Balta","Balta","Balta","Balta","Balta","Balta","Balta","Balta"]
["Matmenys","Įrenginys","","Aukštis","mm","295","295","295","295","295","295","299","299"]
["","","","Plotis","mm","778","778","778","778","778","778","998","998"]
["","","","Gylis","mm","272","272","272","272","272","272","292","292"]
["Svoris","Įrenginys","","","kg","10","10","10","10","10","10","14.5","14.5"]
["Ventiliatorius","Oro debitas","Aušinimas","Didelis","m³/min.","10.5","10.5","11.3","11.3","11.9","11.9","15.8","16.7"]
["","Oro srauto greitis","Vėsinimas","Vidutinis","m³/min.","7.5","7.5","7.8","7.8","9","9","14","14"]
["","","","Mažas","m³/min.","5.7","5.7","6","6","6.5","6.5","11.4","11.8"]
["","","","Tylus veikimas","m³/min.","4.3","4.3","4.2","4.2","4.3","4.3","8.3","9.1"]
["","","Šildymas","Didelis","m³/min.","9.3","9.3","9.8","9.8","12.4","12.4","15.8","16.5"]
["","Oro srauto greitis","Šildymas","Vidutinis","m³/min.","8.2","8.2","8.5","8.5","9.7","9.7","14.2","15.2"]
["","","Šildymas","Mažas","m³/min.","6.2","6.2","6.5","6.5","6.5","6.5","12","12.4"]
["","","","Tylus veikimas","m³/min.","5.1","5.1","4.9","4.9","4.9","4.9","10.5","11.1"]
["Garso galingumo lygis","Vėsinimas","","","dBA","57","57","58","58","60","60","58","60"]
["","Šildymas","","","dBA","54","54","54","54","60","60","58","59"]
["Garso slėgio lygis","Aušinimas","","Aukštas","dBA","41","41","45","45","45","45","44","46"]
["","Vėsinimas","","Vidutinis","dBA","33","33","33","33","39","39","40","42"]
["","","","Žemas","dBA","25","25","29","29","30","30","36","37"]
["","","","Tylus veikimas","dBA","19","19","19","19","21","21","27","30"]
["","Šildymas","","Aukštas","dBA","39","39","39","39","45","45","43","45"]
["","","","Vidutinis","dBA","34","34","35","35","39","39","39","41"]
["","","","Žemas","dBA","26","26","28","28","29","29","34","36"]
["","","","Tylus veikimas","dBA","20","20","20","20","21","21","31","33"]
["Vamzdžių jungtys","Skystis","","OD","mm","6.35","6.35","6.35","6.35","6.35","6.35","6.35","6.35"]
["","Dujos","","Iš. diam.","mm","9.5","9.5","9.5","9.5","9.5","9.5","12.7","12.7"]
["","Drenažas","","","","18","18","18","18","18","18","18","18"]
["Valdymo sistemos","Nuotolinis infraraudonųjų spindulių pultelis","","","","ARC466A67","ARC466A67","ARC466A67","ARC466A67","ARC466A67","ARC466A67","ARC466A67","ARC466A67"]
["","Laidinis nuotolinio valdymo pultelis","","","","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1"]
["Standartiniai priedai","Installation manual","","","","1","1","1","1","1","1","1","1"]
["","Wireless remote control","","","","1","1","1","1","1","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2","2","2","2","2","2"]
["","WLAN adapter kit","","","","1","1","1","1","1","1","1","1"]
["","Operation manual","","","","1","1","1","1","1","1","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1","1","1","1","1","2","2"]
["","Indoor unit fixing screws","","","","2","2","2","2","2","2","2","2"]
["","Mounting plate","","","","1","1","1","1","1","1","1","1"]
["","Remote control holder","","","","1","1","1","1","1","1","1","1"]
["El. tiekimas","Pavadinimas","","","","V1","V1","V1","V1","V1","V1","V1","V1"]
["","Fazė","","","","1~","1~","1~","1~","1~","1~","1~","1~"]
["Maitinimas","Dažnis","","","Hz","50","50","50","50","50","50","50","50"]
["","Įtampa","","","V","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]
["Standartiniai priedai","Silver particle filter","","","","","","","","","","1","1"]